{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-A8"]
[]
[]
[]
[]
["","","","","","2MXM50A2V1B8","2MXM68A2V1B8"]
["Dimensões","Unidade","","Altura","mm","552","734"]
["","","","Largura","mm","852","974"]
["","","","Profundidade","mm","350","408"]
["Peso","Unidade","","","kg","41","60"]
["Compressor","Tipo","","","","Compressor oscilante hermético","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","° CBs","-10","-10"]
["","","","Máx.","° CBs","50","50"]
["Nível de pressão sonora","Arrefecimento","","Nom.","dBA","48","48"]
["","Aquecimento","","Nom.","dBA","50","48"]
["Fluido frigorigéneo","Tipo","","","","R-32","R-32"]
["","Carga","","","kg","1.15","2.00"]
["","Carga","","","tCO2Eq","0.78","1.35"]
["","GWP","","","","675","675"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","20 (1)","25 (1)"]
["","Carga de refrigerante adicional","","","kg/m","0,02 (para comprimento de tubagem superior a 20m)","0,02 (para comprimento de tubagem superior a 30m)"]
["","Diferença de nível","IU - OU","Máx.","m","15","15"]
["","","IU - IU","Máx.","m","7.5","7.5"]
["","Comprimento total da tubagem","Sistema","Real","m","30","50"]
["Acessórios standard","Installation manual","","","","1","1"]
["","Drain cap","","","","","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Alimentação elétrica","Fase","","","","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50"]
["","Tensão","","","V","220-240","220-240"]
["Notas","","","","","(1) - Para uma divisão","(1) - Para uma divisão"]
["","","","","","(2) - Para combinação com CVXM-A, FVXM-A - o comprimento máximo da tubagem é 30 m.","(2) - Para combinação com CVXM-A, FVXM-A - o comprimento máximo da tubagem é 30 m."]
["","","","","","(3) - Consulte o esquema separado para conhecer os limites de funcionamento","(3) - Consulte o esquema separado para conhecer os limites de funcionamento"]
["","","","","","(4) - Consulte o esquema separado para conhecer os dados eléctricos","(4) - Consulte o esquema separado para conhecer os dados eléctricos"]
["","","","","","(5) - Contém gases fluorados com efeito de estufa","(5) - Contém gases fluorados com efeito de estufa"]