{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-N"]
[]
[]
[]
[]
["","","","","","2MXM40N2V1B","2MXM50N2V1B","2MXM68N2V1B"]
["Dimensões","Unidade","","Altura","mm","550","550","734"]
["","","","Largura","mm","765","765","958"]
["","","","Profundidade","mm","285","285","340"]
["Peso","Unidade","","","kg","36","41","60"]
["Motor do ventilador","Velocidade","Arrefecimento","Super baixa","rpm","500","500","420"]
["","","Aquecimento","Super baixa","rpm","320","500","420"]
["Compressor","Tipo","","","","Compressor oscilante hermético","Compressor oscilante hermético","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","° CBs","","","-10"]
["","","","Máx.","° CBs","","","46"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","46","48"]
["","","","Nom.","dBA","","","48"]
["","Aquecimento","","Alto","dBA","48","50"]
["","","","Nom.","dBA","","","48.0"]
["Fluido frigorigéneo","Tipo","","","","R-32","R-32","R-32"]
["","Carga","","","kg","0.88","1.15","2"]
["","Carga","","","tCO2Eq","0.60","0.78","1.35"]
["","GWP","","","","675","675","675.0"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","20","20","25"]
["","Carga de refrigerante adicional","","","kg/m","0,02 (para comprimento de tubagem superior a 20m)","0,02 (para comprimento de tubagem superior a 20m)","0,02 (para comprimento de tubagem superior a 30m)"]
["","Diferença de nível","IU - OU","Máx.","m","15.0","15.0","15.0"]
["","","IU - IU","Máx.","m","7.5","7.5","7.5"]
["","Comprimento total da tubagem","Sistema","Real","m","30","30","50"]
["Acessórios standard","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Alimentação elétrica","Fase","","","","1~","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50","50"]
["","Tensão","","","V","220-230-240","220-230-240","220-240"]
["Notas","","","","","(1) - Para uma divisão","(1) - Para uma divisão","(1) - Para uma divisão"]
["Acessórios standard","Reducer assembly","","","","","1","1"]
["","Drain cap","","","","","","3"]