{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-N"]
[]
[]
[]
[]
["","","","","","4MXM68N2V1B (Archived)","4MXM80N2V1B (Archived)"]
["Ventilador","Caudal de ar","Arrefecimento","Super baixa","m³/min","24.1","24.1"]
["","","Aquecimento","Super baixa","m³/min","24.1","24.1"]
["","","","Super baixa","cfm","851","851.0"]
["","","Aquecimento","Super baixa","cfm","851.0","851.0"]
["Dimensões","Unidade","","Altura","mm","734","734"]
["","","","Largura","mm","958","958"]
["","","","Profundidade","mm","340","340"]
["Peso","Unidade","","","kg","63","67"]
["Compressor","Type","","","","Compressor oscilante hermético","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","°CBs","-10","-10"]
["","","","Máx.","°CBs","46","46"]
["","Aquecimento","Ambiente","Mín.","° CBh","-15","-15"]
["","","","Máx.","° CBh","18","18"]
["Nível de pressão sonora","Arrefecimento","","Nom.","dBA","48","49"]
["","Aquecimento","","Nom.","dBA","48","49"]
["Fluido frigorigéneo","Tipo","","","","R-32","R-32"]
["","Carga","","","kg","2.00","2.40"]
["","Carga","","","tCO2Eq","1.4","1.6"]
["","GWP","","","","675","675"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","25","25"]
["","Carga de refrigerante adicional","","","kg/m","0,02 (para comprimento de tubagem superior a 30m)","0,02 (para comprimento de tubagem superior a 30m)"]
["","Diferença de nível","IU - OU","Máx.","m","15","15"]
["","","IU - IU","Máx.","m","7.5","7.5"]
["","Comprimento total da tubagem","Sistema","Real","m","60","70"]
["Acessórios standard","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Alimentação elétrica","Fase","","","","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50"]
["","Tensão","","","V","220-240","220-240"]