{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXS-E"]
[]
[]
[]
[]
["","","","","","4MXS80E3V3B","4MXS80E3V3B2","4MXS80E7V3B"]
["Dimensões","Unidade","","Altura","mm","770","770"]
["","","","Largura","mm","900","900"]
["","","","Profundidade","mm","320","320"]
["Peso","Unidade","","","kg","72","72"]
["Compressor","Type","","","","Compressor oscilante hermético","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","° CBs","-10","-10"]
["","","","Máx.","° CBs","46","46"]
["","Aquecimento","Ambiente","Mín.","° CBh","-15","-15"]
["","","","Máx.","° CBh","18","18"]
["Nível de pressão sonora","Arrefecimento","","Nom.","dBA","48","48"]
["","Aquecimento","","Nom.","dBA","49","49"]
["Fluido frigorigéneo","Tipo","","","","R-410A","R-410A"]
["","Charge","","","kg","2.99","2.99"]
["","GWP","","","","2,087.5","2,087.5"]
["Ligações de tubagem","Carga de refrigerante adicional","","","kg/m","0,02 (para comprimento de tubagem superior a 30m)","0,02 (para comprimento de tubagem superior a 30m)"]
["","Diferença de nível","IU - OU","Máx.","m","15","15"]
["","","IU - IU","Máx.","m","7.5","7.5"]
["","Comprimento total da tubagem","Sistema","Real","m","70","70"]
["Acessórios standard","Manual de instalação","","","","1","1"]
["","Tampão de drenagem","","","","1","1"]
["","Redutor","","","","1","1"]
["Power supply","Phase","","","","1~","1~"]
["","Frequência","","","Hz","50","50"]
["","Tensão","","","V","230","230"]
["Notas","","","","","(1) - Arrefecimento: temp. interior: 27°CBs, 19,0°CBh; temp. exterior 35°CBs; comprimento de tubagem equivalente: 7.5m","(1) - Arrefecimento: temp. interior: 27°CBs, 19,0°CBh; temp. exterior 35°CBs; comprimento de tubagem equivalente: 7.5m"]
["","","","","","(2) - Aquecimento: temp. interior: 20°CBs; temp. exterior 7°CBs, 6°CBh; tubagem de refrigerante equivalente: 7,5m","(2) - Aquecimento: temp. interior: 20°CBs; temp. exterior 7°CBs, 6°CBh; tubagem de refrigerante equivalente: 7,5m"]
["","","","","","(3) - Contém gases fluorados com efeito de estufa","(3) - Contém gases fluorados com efeito de estufa"]
["Dimensões","Unidade","","Altura","mm","","","770"]
["","","","Largura","mm","","","900"]
["","","","Profundidade","mm","","","320"]
["Peso","Unidade","","","kg","","","72"]
["Compressor","Type","","","","","","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","° CBs","","","-10"]
["","","","Máx.","° CBs","","","46"]
["","Aquecimento","Ambiente","Mín.","° CBh","","","-15"]
["","","","Máx.","° CBh","","","15.5"]
["Nível de pressão sonora","Arrefecimento","","Nom.","dBA","","","48"]
["","Aquecimento","","Nom.","dBA","","","49"]
["Fluido frigorigéneo","Tipo","","","","","","R-410A"]
["","Carga","","","kg","","","2.99"]
["","Carga","","","tCO2Eq","","","6.2"]
["","GWP","","","","","","2087.5"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","","","25"]
["","Carga de refrigerante adicional","","","kg/m","","","0,02 (para comprimento de tubagem superior a 30m)"]
["","Diferença de nível","IU - OU","Máx.","m","","","15"]
["","","IU - IU","Máx.","m","","","7.5"]
["","Comprimento total da tubagem","Sistema","Real","m","","","70"]
["Acessórios standard","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Alimentação elétrica","Fase","","","","","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","","","50"]
["","Tensão","","","V","","","230"]