{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-A"]
[]
[]
[]
[]
["","","","","","5MXM90A2V1B"]
["Dimensões","Unidade","","Altura","mm","734"]
["","","","Largura","mm","974"]
["","","","Profundidade","mm","408"]
["Peso","Unidade","","","kg","68"]
["Compressor","Tipo","","","","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","° CBs","-10"]
["","","","Máx.","° CBs","46"]
["Nível de pressão sonora","Arrefecimento","","Nom.","dBA","52"]
["","Aquecimento","","Nom.","dBA","52"]
["Fluido frigorigéneo","Tipo","","","","R-32"]
["","Carga","","","kg","2.4"]
["","Carga","","","tCO2Eq","1.62"]
["","GWP","","","","675"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","25 (1)"]
["","Carga de refrigerante adicional","","","kg/m","0,02 (para comprimento de tubagem superior a 30m)"]
["","Diferença de nível","IU - OU","Máx.","m","15"]
["","","IU - IU","Máx.","m","7.5"]
["","Comprimento total da tubagem","Sistema","Real","m","75"]
["Acessórios standard","Installation manual","","","","1"]
["","Drain cap","","","","3"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Alimentação elétrica","Fase","","","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50"]
["","Tensão","","","V","220-240"]
["Notas","","","","","(1) - Para uma divisão"]