{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Nível de pressão sonora","Aquecimento","","Alto","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["","","","Funcionamento silencioso","dBA","","36","","41"]
["","","","B","dBA","","38","","43"]
["","Arrefecimento","","Funcionamento silencioso","dBA","","36","","41"]
["","","","B","dBA","","38","","43"]
["","","","Alto","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["Acessórios standard","Manual de instalação","","","","","Manual de instalação","","Manual de instalação"]
["","Manual de funcionamento","","","","","Manual de funcionamento","","Manual de funcionamento"]
["","Parafusos","","","","","Parafusos","","Parafusos"]
["","Anilha","","","","","Anilha","","Anilha"]
["","Controle remoto sem fios","","","","","Controle remoto sem fios","","Controle remoto sem fios"]
["","Grelha de bloqueio da tampa","","","","","Grelha de bloqueio da tampa","","Grelha de bloqueio da tampa"]
["","Bateria","","","","","Bateria","","Bateria"]
["Sistemas de controlo","Controlo remoto por cabo","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Ligações de tubagem","Líquido","","DE","mm","","9.52","","9.52"]
["","Gás","","DE","mm","","15.88","","15.88"]
["","Esgoto","","","","","19.05","","19.05"]
["Potência nominal","Arrefecimento","","Nom.","kW","","0.094","","0.137"]
["","Aquecimento","","Nom.","kW","","0.094","","0.137"]
["Nível de potência sonora","Arrefecimento","","","dBA","","56","","60"]
["","Aquecimento","","","dBA","","56","","60"]
["Dimensões","Unidade","","Largura","mm","","820","","820"]
["","","","Profundidade","mm","","820","","820"]
["","","","Altura","mm","","300","","300"]
["Envolvente","Material","","","","","Aço galvanizado","","Aço galvanizado"]
["Peso","Unidade","","","kg","","39","","39"]
["Ventilador","Caudal de ar","Aquecimento","Alto","m³/min","","29.2","","34.0"]
["","","","B","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","Arrefecimento","B","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","","Alto","m³/min","","29.2","","34.0"]
["","","","Funcionamento silencioso","m³/min","","17.6","","22.1"]
["","","Arrefecimento","Funcionamento silencioso","m³/min","","17.6","","22.1"]
["Painel decorativo","Peso","","","kg","","4","","4"]
["","Dimensões","","Altura","mm","","82","","82"]
["","","","Profundidade","mm","","990","","990"]
["","","","Largura","mm","","990","","990"]
["","Cor","","","","","Branco","","Branco"]
["Power supply","Fase","","","","","1~","","1~"]
["","Nome","","","","","V1","","V1"]
["","Frequência","","","Hz","","50","","50"]
["","Tensão","","","V","","220-240","","220-240"]
["Ventilador","Caudal de ar","Aquecimento","Funcionamento silencioso","m³/min","15","","22.1"]
["Potência nominal","Aquecimento","","Nom.","kW","0.067","","0.137"]
["","Arrefecimento","","Nom.","kW","0.067","","0.137"]
["Ventilador","Caudal de ar","Arrefecimento","Funcionamento silencioso","m³/min","15","","22.1"]
["Envolvente","Material","","","","Aço galvanizado","","Aço galvanizado"]
["Dimensões","Unidade","","Altura","mm","265","","300"]
["","","","Largura","mm","820","","820"]
["","","","Profundidade","mm","820","","820"]
["Peso","Unidade","","","kg","31","","39"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","B","m³/min","17.6","","26.3"]
["","","Aquecimento","Alto","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","B","m³/min","17.6","","26.3"]
["Nível de potência sonora","Arrefecimento","","","dBA","54","","60"]
["","Aquecimento","","","dBA","54","","60"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","B","dBA","35","","43"]
["","","","Funcionamento silencioso","dBA","32","","41"]
["","Aquecimento","","Alto","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","B","dBA","35","","43"]
["","","","Funcionamento silencioso","dBA","32","","41"]
["Ligações de tubagem","Líquido","","DE","mm","9.52","","9.52"]
["","Gás","","DE","mm","15.88","","15.88"]
["","Esgoto","","","","19.05","","19.05"]
["Painel decorativo","Dimensões","","Altura","mm","82","","82"]
["","","","Largura","mm","990","","990"]
["","","","Profundidade","mm","990","","990"]
["","Peso","","","kg","4","","4"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","ARCWLA","","ARCWLA"]
["","Controlo remoto por cabo","","","","ARCWB","","ARCWB"]
["Acessórios standard","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Alimentação elétrica","Fase","","","","1~","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","","50"]
["","Tensão","","","V","220-240","","220-240"]