{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-A8"]
[]
[]
[]
[]
["","","","","","ARXM50A5V1B8"]
["Dimensões","Unidade","","Altura","mm","610"]
["","","","Largura","mm","923"]
["","","","Profundidade","mm","367"]
["Peso","Unidade","","","kg","40"]
["Motor do ventilador","Velocidade","Arrefecimento","Super baixa","rpm","600"]
["Compressor","Tipo","","","","Compressor oscilante hermético"]
["Limite de funcionamento","Arrefecimento","Ambiente","Mín.","°CBs","-10"]
["","","","Máx.","°CBs","50 (1), 46 (1)"]
["","Aquecimento","Ambiente","Mín.","° CBh","-21 (1), -15 (1)"]
["","","","Máx.","° CBh","18"]
["Nível de pressão sonora","Arrefecimento","","Nom.","dBA","48"]
["","Aquecimento","","Nom.","dBA","49"]
["Fluido frigorigéneo","Tipo","","","","R-32"]
["","Carga","","","kg","0.95"]
["","Carga","","","tCO2Eq","0.65"]
["","GWP","","","","675"]
["Ligações de tubagens","Comprimento da tubagem","Máx.","OU - IU","m","30"]
["","Carga de refrigerante adicional","","","kg/m","0,02 (para comprimento de tubagem superior a 10m)"]
["","Diferença de nível","IU - OU","Máx.","m","20"]
["Acessórios standard","Installation manual","","","","1"]
["","Drain joint","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","LOT10 Energy Label","","","","1"]
["","Drain cap","","","","3"]
["Alimentação elétrica","Fase","","","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50"]
["","Tensão","","","V","220-240"]
["Notas","","","","","(1) - Consulte o esquema separado para conhecer os limites de funcionamento"]
["","","","","","(2) - Consulte o esquema separado para conhecer os dados eléctricos"]
["","","","","","(3) - Contém gases fluorados com efeito de estufa"]