{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":11,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B","ATXF25A5V1B (Archived)","ATXF35A5V1B (Archived)"]
["Nível de pressão sonora","Aquecimento","","Alto","dBA","40","42","44","45"]
["","","","Médio","dBA","34","38","40","41"]
["","","","Funcionamento silencioso","dBA","21","30","32","33"]
["","","","B","dBA","28","33","35","36"]
["","Arrefecimento","","Medium","dBA","33","39","41","42"]
["","","","Funcionamento silencioso","dBA","20","31","33","34"]
["","","","B","dBA","26","34","36","37"]
["","","","Alto","dBA","40","43","45","46"]
["Acessórios standard","Manual de instalação","","","","1","1","1","1"]
["","Manual de funcionamento","","","","1","1","1","1"]
["","Controle remoto por infravermelhos","","","","1","1","1","1"]
["","Pilhas secas AAA","","","","2","2","2","2"]
["","Suporte do controle remoto","","","","1","1","1","1"]
["","Chapa de montagem","","","","1","1","1","1"]
["","Parafusos de fixação da unidade interior","","","","2","2","2","2"]
["Sistemas de controlo","Wired remote control","","","","BRC944B2, BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["","Controlo remoto por infravermelhos","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35"]
["","Gás","","OD","mm","9.50","12.7","12.7","12.7"]
["","Drain","","","","18","18","18","18"]
["Power input","Arrefecimento","","Nom.","kW","0.019","0.029","0.032","0.032"]
["","Aquecimento","","Nom.","kW","0.020","0.032","0.035","0.035"]
["Nível de potência sonora","Arrefecimento","","","dBA","55","59","60","62"]
["","Aquecimento","","","dBA","55","61","62","62"]
["Dimensões","Unidade","","Width","mm","770","990","990","990"]
["","","","Depth","mm","225","263","263","263"]
["","","","Altura","mm","286","295","295","295"]
["Envolvente","Cor","","","","Branco","Branco","Branco","Branco"]
["Peso","Unidade","","","kg","8.50","13.5","13.5","13.5"]
["Ventilador","Caudal de ar","Aquecimento","Alto","m³/min","10.3","17.3","17.9","17.9"]
["","","","B","m³/min","6.7","12.2","12.8","12.8"]
["","","","Medium","m³/min","8.6","14.8","15.8","15.8"]
["","","","Funcionamento silencioso","m³/min","5.3","10.7","11.3","11.3"]
["","","Arrefecimento","B","m³/min","6.1","11.9","12.2","12.2"]
["","","","Medium","m³/min","8.1","14.4","14.8","14.8"]
["","","","Alto","m³/min","10.1","16.8","17.3","17.3"]
["","","","Funcionamento silencioso","m³/min","4.4","10.5","10.7","10.7"]
["Power supply","Fase","","","","1~","1~","1~","1~"]
["","Frequência","","","Hz","50","50","50","50"]
["","Nome","","","","","V1","V1","V1"]
["","Tensão","","","V","220-240","220-240","220-240","220-240"]
["Potência nominal","Arrefecimento","","Nom.","kW","","","","","0.019","0.032"]
["","Aquecimento","","Nom.","kW","","","","","0.02","0.032"]
["Envolvente","Cor","","","","","","","","Branco","Branco"]
["Dimensões","Unidade","","Altura","mm","","","","","286","286"]
["","","","Largura","mm","","","","","770","770"]
["","","","Profundidade","mm","","","","","225","225"]
["Peso","Unidade","","","kg","","","","","8.5","9"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","","","","","10.1","11.5"]
["","","","Médio","m³/min","","","","","8.1","8.3"]
["","","","B","m³/min","","","","","6.1","6.3"]
["","","","Funcionamento silencioso","m³/min","","","","","4.4","4.5"]
["","","Aquecimento","Alto","m³/min","","","","","10.3","11.5"]
["","","","Médio","m³/min","","","","","8.6","9"]
["","","","B","m³/min","","","","","6.7","7"]
["","","","Funcionamento silencioso","m³/min","","","","","5.3","5.3"]
["Nível de potência sonora","Arrefecimento","","","dBA","","","","","55","58"]
["","Aquecimento","","","dBA","","","","","55","58"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","","","","","40","43"]
["","","","Médio","dBA","","","","","33","34"]
["","","","B","dBA","","","","","26","27"]
["","","","Funcionamento silencioso","dBA","","","","","20","20"]
["","Aquecimento","","Alto","dBA","","","","","40","40"]
["","","","Médio","dBA","","","","","34","35"]
["","","","B","dBA","","","","","28","29"]
["","","","Funcionamento silencioso","dBA","","","","","21","21"]
["Ligações de tubagem","Líquido","","DE","mm","","","","","6.35","6.35"]
["","Gás","","DE","mm","","","","","9.5","9.5"]
["","Esgoto","","","","","","","","18","18"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","","","","","ARC470A1","ARC470A1"]
["","Controlo remoto por cabo","","","","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Acessórios standard","Installation manual","","","","","","","","1","1"]
["","AAA dry-cell batteries","","","","","","","","2","2"]
["","Operation manual","","","","","","","","1","1"]
["","Indoor unit fixing screws","","","","","","","","2","2"]
["","Infrared remote control","","","","","","","","1","1"]
["","Mounting plate","","","","","","","","1","1"]
["","Remote control holder","","","","","","","","1","1"]
["Alimentação elétrica","Fase","","","","","","","","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","","","","","50","50"]
["","Tensão","","","V","","","","","220-240","220-240"]