{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-N"]
[]
[]
[]
[]
["","","","","","ATXP20N5V1B","ATXP25N5V1B"]
["Potência nominal","Arrefecimento","","Nom.","kW","0.019","0.02"]
["","Aquecimento","","Nom.","kW","0.023","0.023"]
["Envolvente","Cor","","","","Branco","Branco"]
["Dimensões","Unidade","","Altura","mm","286","286"]
["","","","Largura","mm","770","770"]
["","","","Profundidade","mm","225","225"]
["Peso","Unidade","","","kg","8.5","8.5"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","9.5","9.7"]
["","","","Médio","m³/min","7.4","7.7"]
["","","","B","m³/min","5.6","5.8"]
["","","","Funcionamento silencioso","m³/min","4.2","4.2"]
["","","Aquecimento","Alto","m³/min","10.4","10.4"]
["","","","Médio","m³/min","8.1","8.1"]
["","","","B","m³/min","6.2","6.4"]
["","","","Funcionamento silencioso","m³/min","5.2","5.2"]
["Nível de potência sonora","Arrefecimento","","","dBA","55","55"]
["","Aquecimento","","","dBA","55","55"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","39","40"]
["","","","Médio","dBA","33","33"]
["","","","B","dBA","25","26"]
["","","","Funcionamento silencioso","dBA","19","19"]
["","Aquecimento","","Alto","dBA","39","40"]
["","","","Médio","dBA","34","34"]
["","","","B","dBA","28","28"]
["","","","Funcionamento silencioso","dBA","21","21"]
["Ligações de tubagem","Líquido","","DE","mm","6","6"]
["","Gás","","DE","mm","9.5","9.5"]
["","Esgoto","","","","18","18"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","ARC480A78","ARC480A78"]
["","Controlo remoto por cabo","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Acessórios standard","Installation manual","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Alimentação elétrica","Fase","","","","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50"]
["","Tensão","","","V","220-240","220-240"]