{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AVA-A"]
[]
[]
[]
[]
["","","","","","AVA125AMVE"]
["Capacidade de arrefecimento","Capacidade total","","Nom.","kW","12.10"]
["Capacidade de aquecimento","Capacidade total","","Nom.","kW","13.5"]
["Envolvente","Cor","","","","Branco fresco"]
["Dimensões","Unidade","","Altura","mm","1850"]
["","","","Largura","mm","600"]
["","","","Profundidade","mm","350"]
["Peso","Unidade","","","kg","50"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","28"]
["","","","Médio","m³/min","26"]
["","","","B","m³/min","24"]
["","","Aquecimento","Alto","m³/min","28"]
["","","","Médio","m³/min","26"]
["","","","B","m³/min","24"]
["Nível de potência sonora","Arrefecimento","","","dBA","63"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","51"]
["","","","Médio","dBA","48"]
["","","","B","dBA","46"]
["","Aquecimento","","Alto","dBA","51"]
["","","","Médio","dBA","46"]
["","","","Nom.","dBA","48"]
["Ligações de tubagem","Líquido","","DE","mm","9.52"]
["","Gás","","DE","mm","15.9"]
["","Esgoto","","","","I.D. 20/O.D. 26"]
["Sistemas de controlo","Controlo remoto por cabo","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Acessórios standard","Installation manual","","","","1"]
["","Hole protection rubber","","","","2"]
["","Cover","","","","1"]
["","Dew proof material","","","","1"]
["","Remote control wiring","","","","1"]
["","Bracket for installation","","","","1"]
["","Operation manual","","","","1"]
["","Bush","","","","1"]
["","Installation pattern","","","","1"]
["","Insulation for fitting for gas pipe","","","","1"]
["","Insulation for fitting for liquid pipe","","","","1"]
["","Screws","","","","5"]
["","Tie-wraps","","","","5"]
["Alimentação elétrica","Fase","","","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50/60"]
["","Tensão","","","V","220-240/220"]