{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1E53A"]
[]
[]
[]
[]
["","","","","BRC1E53A7"]
["Envolvente","Cor","","","Branco fresco"]
["","Tampa do botão","","","Não"]
["","LED de funcionamento","Cor","","Verde"]
["Dimensões","Unidade","Altura","mm","120"]
["","","Width","mm","120"]
["","","Depth","mm","19"]
["","Unidade embalada","Altura","mm","55"]
["","","Largura","mm","160"]
["","","Profundidade","mm","150"]
["Peso","Unidade","","kg","0.200"]
["","Unidade embalada","","kg","0.415"]
["Acondicionamento","Material","","","Cartão_"]
["","Peso","","kg","0.05"]
["LCD","Tipo","","","Ponto completo (160 x 255)"]
["","Dimensões","Altura","mm","43.2"]
["","","Largura","mm","68.85"]
["","Retroiluminação","Cor","","Branco"]
["Temperatura ambiente","Funcionamento","Mín.","°C","-10"]
["","","Máx.","°C","50"]
["","Armazenamento","Mín.","°C","-20"]
["","","Máx.","°C","70"]
["","Humidade relativa <","","%","95"]
["Wiring connections","Comprimento da cablagem","Máx.","m","500"]
["Reserva para falha de energia","","","","Sim (o relógio continuará a funcionar durante um período não superior a 48 horas)"]