{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1H52S"]
[]
[]
[]
[]
["","","","","BRC1H52S."]
["Acondicionamento","Material","","","Cartão"]
["","Peso","","kg","0.0850"]
["Temperatura ambiente","Humidade relativa <","","%","95"]
["","Armazenamento","Mín.","°C","-20"]
["","","Máx.","°C","70"]
["","Funcionamento","Mín.","°C","-10"]
["","","Máx.","°C","50"]
["Dimensões","Unidade embalada","Largura","mm","217"]
["","","Altura","mm","50"]
["","","Profundidade","mm","161"]
["","Unidade","Width","mm","85"]
["","","Depth","mm","25"]
["","","Altura","mm","85"]
["Envolvente","Tampa do botão","","","Não"]
["","Cor","","","Prateado"]
["","LED de funcionamento","Cor","","Blue status indicator"]
["LCD","Tipo","","","100 x 150 dots"]
["","Retroiluminação","Cor","","Branco"]
["","Dimensões","Largura","mm","28.0"]
["","","Altura","mm","40.7"]
["Peso","Unidade embalada","","kg","0.317"]
["","Unidade","","kg","0.110"]
["Wiring connections","Comprimento da cablagem","Máx.","m","500"]