{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC2E52C"]
[]
[]
[]
[]
["","","","","BRC2E52C7"]
["Acondicionamento","Material","","","Cartão_"]
["","Peso","","kg","0.050"]
["Temperatura ambiente","Humidade relativa <","","%","95"]
["Dimensões","Unidade embalada","Largura","mm","160"]
["","","Altura","mm","150"]
["","","Profundidade","mm","55"]
["","Unidade","Largura","mm","120"]
["","","Profundidade","mm","19"]
["","","Altura","mm","120"]
["Envolvente","Tampa do botão","","","Não"]
["","Cor","","","Branco fresco"]
["","Operation LED","Colour","","Verde"]
["LCD","Tipo","","","Ponto completo (160 x 255)"]
["","Retroiluminação","Cor","","Branco"]
["","Dimensões","Largura","mm","68.85"]
["","","Altura","mm","43.2"]
["Peso","Unidade embalada","","kg","0.415"]
["","Unidade","","kg","0.200"]
["Reserva para falha de energia","","","","Sim (o relógio continuará a funcionar durante um período não superior a 48 horas)"]
["Ligações eléctricas","Comprimento da cablagem","Máx.","m","500"]