{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 5MXM-N"]
[]
[]
[]
[]
["","","","","","CHYHBH08AAV32 / 5MXM90N2V1B","CHYHBH05AAV32 / 5MXM90N2V1B","CHYHBH05AFV32 / 5MXM90N2V1B","CHYHBH08AFV32 / 5MXM90N2V1B"]
["Aquecimento de água quente sanitária","Geral","","Perfil de carga declarado","","XL","XL"]
["","Clima médio","","Classe de eficiência energética para aquecimento de água","","A","A"]
["COP","","","","","4.17 (1)","4.04 (1)","4.04","4.17"]
["Aquecimento de espaços","Clima médio, saída da água 55 °C","Geral","Seasonal space heating eff. class","","A+","A+"]
["","","","ηs (Eficiência sazonal de aquecimento de espaços)","%","120.8","120.8"]
["","","","SCOP","","3.09","3.09"]
["Capacidade de aquecimento","Nom.","","","kW","6.78 (1)","4.50 (1)"]
["Notas","","","","","(1) - Bs/Bh 7 °C/6 °C - LWC 35 °C (DT=5 °C), caldeira derivada","(1) - Bs/Bh 7 °C/6 °C - LWC 35 °C (DT=5 °C), caldeira derivada","(1) - Bs/Bh 7 °C/6 °C - LWC 35 °C (DT=5 °C), caldeira derivada","(1) - Bs/Bh 7 °C/6 °C - LWC 35 °C (DT=5 °C), caldeira derivada"]
["Capacidade de aquecimento","Nom.","","","kW","","","4.5","6.78"]
["Aquecimento de água quente sanitária","Geral","","Perfil de carga declarado","","","","XL","XL"]
["","Clima médio","","Classe de eficiência energética para aquecimento de água","","","","A","A"]
["Aquecimento de espaços","Clima médio, saída da água 55 °C","Geral","SCOP","","","","3.09","3.09"]
["","","","Classe de efic. sazonal de aquecimento de espaços","","","","A+","A+"]
["Gama de eficiência energética","","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]