{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CKHWS-BV3"]
[]
[]
[]
[]
["","","","","","CKHWS180BJV3","CKHWS230BJV3"]
["Dimensões","Unidade","Altura","Depósito","mm","1655","1855"]
["","","","Largura","mm","595","595"]
["","","","Profundidade","mm","634","634"]
["Peso","Unidade","","Vazio","kg","106","115"]
["Depósito","Volume de água","","","l","180","230"]
["","Material","","","","Aço inoxidável (EN 1.4521)","Aço inoxidável (EN 1.4521)"]
["","Temperatura máxima da água","","","°C","65.0","65.0"]
["","Classe de eficiência energética","","","","B","B"]
["Resistência de apoio","Potência","","","kW","1.5","1.5"]
["Notas","","","","","(1) - Baseado num dT de 45 K","(1) - Baseado num dT de 45 K"]
["","","","","","(2) - Caudal DHW","(2) - Caudal DHW"]
["","","","","","(3) - 2 polos 10 A, curva 230 V","(3) - 2 polos 10 A, curva 230 V"]
["","","","","","(4) - A alimentação eléctrica da hydro box acima referida destina-se apenas ao aquecedor de reserva. A caixa de derivação e a bomba da hydrobox são fornecidas através da unidade exterior.","(4) - A alimentação eléctrica da hydro box acima referida destina-se apenas ao aquecedor de reserva. A caixa de derivação e a bomba da hydrobox são fornecidas através da unidade exterior."]