{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AW"]
[]
[]
[]
[]
["","","","","","CTXA15A2V1BW"]
["Nível de pressão sonora","Aquecimento","","Alto","dBA","39"]
["","","","Médio","dBA","32"]
["","","","Funcionamento silencioso","dBA","21"]
["","","","B","dBA","25"]
["","Arrefecimento","","Medium","dBA","32"]
["","","","Funcionamento silencioso","dBA","21"]
["","","","B","dBA","25"]
["","","","Alto","dBA","39"]
["Acessórios standard","Manual de instalação","","","","1"]
["","Manual de funcionamento","","","","1"]
["","Filtro de ar","","","","2"]
["","Controle remoto por infravermelhos","","","","1"]
["","Placa de instalação do controlador remoto","","","","1"]
["","Saco de parafusos","","","","1"]
["","Tampa do parafuso","","","","1"]
["","Pilhas secas AAA","","","","2"]
["","Precauções gerais de segurança","","","","1"]
["Fluido frigorigéneo","GWP","","","","675.0"]
["Sistemas de controlo","Controlo remoto por cabo","","","","BRC073"]
["","Infrared remote control","","","","ARC466A58"]
["Ligações de tubagens","Liquid","","OD","mm","6.35"]
["","Gás","","OD","mm","9.50"]
["","Drain","","","","18"]
["Power input","Arrefecimento","","Nom.","kW","0.020"]
["","Aquecimento","","Nom.","kW","0.020"]
["Sound power level","Arrefecimento","","","dBA","57"]
["Dimensões","Unidade","","Largura","mm","798"]
["","","","Profundidade","mm","189"]
["","","","Altura","mm","295"]
["Envolvente","Cor","","","","Branco"]
["Peso","Unidade","","","kg","12"]
["Ventilador","Caudal de ar","Aquecimento","Alto","m³/min","10.9"]
["","","","Medium","m³/min","8.7"]
["","","","B","m³/min","6.4"]
["","","","Funcionamento silencioso","m³/min","4.5"]
["","","Arrefecimento","B","m³/min","6.1"]
["","","","Medium","m³/min","8"]
["","","","Alto","m³/min","11.0"]
["","","","Funcionamento silencioso","m³/min","4.6"]
["Power supply","Fase","","","","1~"]
["","Nome","","","","V1"]
["","Frequência","","","Hz","50"]
["","Tensão","","","V","220-240"]