{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-BS"]
[]
[]
[]
[]
["","","","","","CTXA15B2V1BS"]
["Potência nominal","Arrefecimento","","Nom.","kW","0.02"]
["","Aquecimento","","Nom.","kW","0.02"]
["Envolvente","Cor","","","","Prateado"]
["Dimensões","Unidade","","Altura","mm","295"]
["","","","Largura","mm","798"]
["","","","Profundidade","mm","189"]
["Peso","Unidade","","","kg","11.5"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","11"]
["","","","Médio","m³/min","8.2"]
["","","","B","m³/min","6.1"]
["","","","Funcionamento silencioso","m³/min","4.6"]
["","","Aquecimento","Alto","m³/min","10.9"]
["","","","Médio","m³/min","8.7"]
["","","","B","m³/min","6.4"]
["","","","Funcionamento silencioso","m³/min","4.5"]
["Nível de potência sonora","Arrefecimento","","","dBA","57"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","39"]
["","","","Médio","dBA","32"]
["","","","B","dBA","25"]
["","","","Funcionamento silencioso","dBA","21"]
["","Aquecimento","","Alto","dBA","39"]
["","","","Médio","dBA","32"]
["","","","B","dBA","25"]
["","","","Funcionamento silencioso","dBA","21"]
["Fluido frigorigéneo","GWP","","","","675"]
["Ligações de tubagem","Líquido","","DE","mm","6.35"]
["","Gás","","DE","mm","9.5"]
["","Esgoto","","","","18"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","ARC466A58"]
["","Controlo remoto por cabo","","","","BRC073"]
["Acessórios standard","Installation manual","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Filtro de ar","","","","2"]
["","Infrared remote control","","","","1"]
["","Remote controller mounting plate","","","","1"]
["","Screw bag","","","","1"]
["Alimentação elétrica","Nome","","","","V1"]
["","Fase","","","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50"]
["","Tensão","","","V","220-240"]