{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Nível de pressão sonora","Aquecimento","","Alto","dBA","38","","41"]
["","","","Funcionamento silencioso","dBA","21","","21"]
["","","","B","dBA","28","","30"]
["","Arrefecimento","","Funcionamento silencioso","dBA","21","","21"]
["","","","B","dBA","25","","28"]
["","","","Alto","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Arrefecimento","","Nom.","dBA","31","","35"]
["Acessórios standard","Manual de instalação","","","","1","","1"]
["","Manual de funcionamento","","","","1","","1"]
["","Controle remoto sem fios","","","","1","","1"]
["","Pilhas","","","","2","","2"]
["","Suporte do controle remoto","","","","1","","1"]
["","Chapa de montagem","","","","1","","1"]
["","Parafusos de fixação da unidade interior","","","","2","","2"]
["","Filtro fotocatalítico de apatite de titânio","","","","2","","2"]
["Sistemas de controlo","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Ligações de tubagem","Líquido","","DE","mm","6.35","","6.35"]
["","Gás","","DE","mm","9.5","","9.5"]
["","Esgoto","","","","18","","18"]
["Potência nominal","Arrefecimento","","Nom.","kW","0.040","","0.040"]
["","Aquecimento","","Nom.","kW","0.040","","0.040"]
["Nível de potência sonora","Arrefecimento","","","dBA","55","","59"]
["","Aquecimento","","","dBA","56","","58"]
["Dimensões","Unidade","","Largura","mm","780","","780"]
["","","","Profundidade","mm","215","","215"]
["","","","Altura","mm","289","","289"]
["Envolvente","Cor","","","","Branco","","Branco"]
["Peso","Unidade","","","kg","8","","8"]
["Ventoinha","Caudal de ar","Aquecimento","Alto","m³/min","","","10.1"]
["","","","B","m³/min","","","6.3"]
["","","","Funcionamento silencioso","m³/min","","","4.3"]
["","","Arrefecimento","B","m³/min","","","5.2"]
["","","","Alto","m³/min","","","9.2"]
["","","","Funcionamento silencioso","m³/min","","","3.9"]
["","","","Nom.","m³/min","","","8.1"]
["","","Arrefecimento","Nom.","m³/min","","","7.2"]
["Power supply","Fase","","","","1~","","1~"]
["","Frequência","","","Hz","50","","50"]
["","Nome","","","","V1","","V1"]
["","Tensão","","","V","220-240","","220-240"]
["Notas","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Potência nominal","Arrefecimento","","Nom.","kW","","0.04","","0.040"]
["","Aquecimento","","Nom.","kW","","0.04","","0.040"]
["Envolvente","Cor","","","","","Branco","","Branco"]
["Dimensões","Unidade","","Altura","mm","","289","","289"]
["","","","Largura","mm","","780","","780"]
["","","","Profundidade","mm","","215","","215"]
["Peso","Unidade","","","kg","","8","","8.00"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","","7.9","","9.2"]
["","","","Médio","m³/min","","6.3","","7.2"]
["","","","B","m³/min","","4.7","","5.2"]
["","","","Funcionamento silencioso","m³/min","","3.9","","3.9"]
["","","Aquecimento","Alto","m³/min","","9","","10.1"]
["","","","Médio","m³/min","","7.5","","8.1"]
["","","","B","m³/min","","6","","6.3"]
["","","","Funcionamento silencioso","m³/min","","4.3","","4.3"]
["Nível de potência sonora","Arrefecimento","","","dBA","","55","","59"]
["","Aquecimento","","","dBA","","56","","58"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","","37","","42"]
["","","","Médio","dBA","","31","","35"]
["","","","B","dBA","","25","","28"]
["","","","Funcionamento silencioso","dBA","","21","","21"]
["","Aquecimento","","Alto","dBA","","38","","41"]
["","","","Médio","dBA","","33","","36"]
["","","","B","dBA","","28","","30"]
["","","","Funcionamento silencioso","dBA","","21","","21"]
["Ligações de tubagem","Líquido","","DE","mm","","6.35","","6.35"]
["","Gás","","DE","mm","","9.5","","9.50"]
["","Esgoto","","","","","18","","18"]
["Sistemas de controlo","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Acessórios standard","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Alimentação elétrica","Nome","","","","","V1","","V1"]
["","Fase","","","","","1~","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","","50","","50"]
["","Tensão","","","V","","220-240","","220-240"]