{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":11,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2CND-A4A"]
[]
[]
[]
[]
["","","","","","D2CND024A4AB","D2CND024A4AA","D2CND028A4AA","D2CND028A4AB","D2CND035A4AA","D2CND035A4AB"]
["Gás","Consumo (G20)","","Mín","m³/h","0.31","0.31","0.511","0.511","0.511","0.511"]
["","","","Máx.","m³/h","2.48","2.48","2.89","2.89","3.63","3.63"]
["","Consumo (G25)","","Mín","m³/h","0.36","0.36","0.59","0.59","0.59","0.59"]
["","","","Máx.","m³/h","2.89","2.89","3.32","3.32","4.19","4.19"]
["","Consumo (G31)","","Mín","m³/h","0.12","0.12","0.2","0.2","0.2","0.2"]
["","","","Máx.","m³/h","0.96","0.96","1.1","1.1","1.38","1.38"]
["","Classe NOx","","","","6","6","6","6","6","6"]
["","Nível de NOx (G20)","","","mg/kWh","22","22","36.3","36.3","35.5","35.5"]
["Aquecimento central","Qn de entrada de calor (valor calorífico líquido)","Nom","Mín","kW","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Máx.","kW","23.5","23.5","27","27","34","34"]
["","Qn de entrada de calor (valor calorífico bruto)","Nom","Mín","kW","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Máx.","kW","26.1","26.1","30","30","37.8","37.8"]
["","Pn de saída a 80/60°C","","Mín","kW","2.8","2.8","4.6","4.6","4.6","4.6"]
["","","","Nom","kW","22.8","22.8","26.3","26.3","33.2","33.2"]
["","Pnc de saída a 50/30°C","","Mín","kW","3.1","3.1","5.2","5.2","5.2","5.2"]
["","","","Nom","kW","24","24.0","28.2","28.2","35","35"]
["","Saída a 37/30°C","","Nom","kW","7.6","7.6","8.8","8.8","11.1","11.1"]
["","Temperatura da água","","Máx.","°C","100","100","100","100","100","100"]
["","Eficiência","","Valor calorífico líquido","%","97.9","97.9"]
["","","","Valor calorífico bruto","%","87.3","87.3"]
["Água quente sanitária","Qnw de entrada de calor (valor calorífico líquido)","Nom","Mín","kW","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Máx.","kW","23.5","23.5","29.5","29.5","34","34"]
["","Qnw de entrada de calor (valor calorífico bruto)","Nom","Mín","kW","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Máx.","kW","26.1","26.1","32.7","32.7","37.7","37.7"]
["","Temperatura","","Máx.","°C","60","60","60","60","60","60"]
["Perdas de calor","Ps de caldeira em espera","","","kW","0.057","0.057","0.0650","0.065","0.0650","0.065"]
["Ar de alimentação","Ligação","","","mm","100","100","100","100","100","100"]
["","Concêntrico","","","","Sim","Sim","Sim","Sim","Sim","Sim"]
["Gás combustível","Temperatura","","Máx.","°C","90","90","76.4","76.4","81.7","81.7"]
["","Ligação","","","mm","60","60","60","60","60","60"]
["","Caudal mássico (G20)","","Máx.","kg/h","38.7","38.7","44.5","55.7","55.7","55.7"]
["","Caudal mássico (G31)","","Máx.","kg/h","36","36.0","43.3","43.3","54.7","54.7"]
["Envolvente","Cor","","","","Branco titânio (Ral9003)","Branco titânio (Ral9003)","Branco titânio (Ral9003)","Branco titânio (Ral9003)","Branco titânio (Ral9003)","Branco titânio (Ral9003)"]
["","Material","","","","Folha de metal","Folha de metal","Chapa pintada de aço galvanizado","Chapa pintada de aço galvanizado","Chapa pintada de aço galvanizado","Chapa pintada de aço galvanizado"]
["Dimensões","Unidade","Altura","Estrutura","mm","590","590","690","690","690","690"]
["","","","Largura","mm","400","400","440","440","440","440"]
["","","","Profundidade","mm","256","256","295","295","295","295"]
["Peso","Unidade","","Vazio","kg","27","27","37","37","37","37"]
["","","","Total","kg","27","27","39","","39"]
["","Caldeira","","Vazio","kg","27","27.0"]
["Aquecimento de água quente sanitária","Geral","","Perfil de carga declarado","","XL","XL","XL","XL","XL","XL"]
["","","","Classe de eficiência energética de aquecimento de água","","A","A","A","A","A","A"]
["Aquecimento ambiente","Geral","","Classe de eficiência de aquecimento ambiente sazonal","","A","A","A","A","A","A"]
["Gás combustível","Caudal mássico (G25)","","Máx.","kg/h","","","39.3","39.3","49.6","49.6"]