{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Temperatura ambiente","Humidade relativa <","","","%","85"]
["Número máximo de unidades interiores conectáveis","","","","","32"]
["Potência absorvida","kW","","","","0.015 (1)"]
["Comunicação","DIII-NET","","Quantidade","","1"]
["","","","Observação","","DIII-NET (F1F2)"]
["","Ethernet","","Quantidade","","1"]
["","Terminal de entrada","Digital","Quantidade","","4"]
["Dimensões","Unidade","","Largura","mm","384"]
["","","","Profundidade","mm","92"]
["","","","Altura","mm","136"]
["Número máximo de unidades exteriores conectáveis","","","","","7"]
["Power supply","Frequência","","","Hz","50/60"]
["","Tensão","","","V","110-240 CA"]
["Notas","","","","","(1) - Inclui a potência absorvida da fonte de alimentação WAGO, o módulo CPU e o módulo de E/S"]
["","","","","","(2) - As dimensões incluem a fonte de alimentação WAGO, o módulo CPU, o módulo de E/S e o espaço necessário entre as diferentes peças"]
["","","","","","(3) - As dimensões do ecrã opcional são: altura: 209 mm, largura: 123 mm, profundidade: 8,5 mm"]