{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","E1500"]
[]
[]
[]
[]
["","","","","EZESHP20AUAW1B"]
["Potência frigorífica","Refrigerating capacity-=-At 0°C setpoint (30°C Ambient Temperature)","Refrigerating capacity-=-At 0°C setpoint (30°C Ambient Temperature)-=-R-452A-=-kW","kW","14,900"]
["","Refrigerating capacity-=-At -20°C setpoint (30°C Ambient Temperature)","Refrigerating capacity-=-At -20°C setpoint (30°C Ambient Temperature)-=-R-452A-=-kW","kW","9,200"]
["Capacidade de aquecimento","Heating capacity-=-At +2°C setpoint (-20°C Ambient Temperature)","Heating capacity-=-At +2°C setpoint (-20°C Ambient Temperature)-=-R-452A-=-kW","kW","10,500"]
["Potência absorvida","Power input-=-Engine","Power input-=-Engine-=-Type","","Kubota Custom Diesel Engine, 4 Cylinders, NRMM Stage V Compliant"]
["","","Power input-=-Engine-=-Displacement-=-cc","cc","1,500"]
["","","Power input-=-Engine-=-Maintenance interval-=-hr","hr","3,000"]
["","Power input-=-Generator","Power input-=-Generator-=-Type","","Direct Drive"]
["","","Power input-=-Generator-=-Power-=-kW","kW","15"]
["Dimensões","Unidade","Altura","mm","2,227"]
["","","Largura","mm","2,072"]
["","","Profundidade","mm","440"]
["","Unidade embalada","Altura","mm","2,066"]
["","","Largura","mm","2,345"]
["","","Profundidade","mm","542"]
["Peso","Unidade","","kg","730"]
["Compressor","Type","","","Custom Scroll Compressor - Economizer/Inverter"]
["Fluido frigorigéneo","Tipo","","","R-452A"]
["Nível de pressão sonora","Nom.","","dBA","65"]
["Power supply","Tensão","","V","400"]
["","Fase","","","3P+N"]
["","Frequência","","Hz","50"]