{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBLA-D3V37"]
[]
[]
[]
[]
["","","","","","EBLA16DA3V37"]
["Capacidade de aquecimento","Nom.","","","kW","16.0 (2) (1)"]
["Capacidade de arrefecimento","Nom.","","","kW","14.0 (3), 15.3 (4)"]
["Capacidade do aquecedor","Escalão 1","","","kW","3"]
["Potência nominal","Arrefecimento","","Nom.","kW","4.58 (3), 3.24 (4)"]
["","Aquecimento","","Nom.","kW","3.53 (1), 4.56 (2)"]
["COP","","","","","4.53 (1), 3.51 (2)"]
["EER","","","","","3.06 (3), 4.74 (4)"]
["Dimensões","Unidade","","Altura","mm","870"]
["","","","Largura","mm","1380"]
["","","","Profundidade","mm","460"]
["Peso","Unidade","","","kg","149"]
["Ventilador","Caudal de ar","Aquecimento","Alto","m³/min","85.0"]
["","","Arrefecimento","Alto","m³/min","85.0"]
["Limite de funcionamento","Aquecimento","Lado da água","Mín.","°C","15 (6)"]
["","","","Máx.","°C","60 (6)"]
["","Arrefecimento","Ambiente","Mín.","° CBs","10"]
["","","","Máx.","° CBs","43"]
["","","Lado da água","Mín.","°C","5"]
["","","","Máx.","°C","22"]
["","Água doméstica quente","Ambiente","Mín.","° CBs","-25"]
["","","","Máx.","° CBs","35"]
["","","Lado da água","Mín.","°C","25"]
["","","","Máx.","°C","55 (6)"]
["Fluido frigorigéneo","Tipo","","","","R-32"]
["","GWP","","","","675"]
["","Carga","","","kg","3.80"]
["","Carga","","","tCO2Eq","2.57"]
["Aquecimento de espaços","Clima médio, saída da água 55 °C","Geral","SCOP","","3.37"]
["","","","Classe de efic. sazonal de aquecimento de espaços","","A++"]
["","Clima médio, saída da água 35 °C","Geral","SCOP","","4.69"]
["","","","Classe de efic. sazonal de aquecimento de espaços","","A+++"]
["Componente do compressor","Alimentação eléctrica principal","","Fase","","1"]
["","","","Tensão","V","230"]
["Alimentação elétrica","Nome","","","","V3"]
["","Fase","","","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50"]
["","Tensão","","","V","230"]
["Notas","","","","","(1) - Condição: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condição: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(3) - Arrefecimento: AE 12℃; AS 7℃; condições ambiente: 35°CBs"]
["","","","","","(4) - Arrefecimento: AE 23℃; AS 18℃; condições ambiente: 35°CBs"]
["","","","","","(5) - Em conformidade com a EN14825"]
["","","","","","(6) - Para mais informações, consulte o desenho dos limites de funcionamento"]
["","","","","","(7) - Depende do modo de funcionamento, consulte o manual de instalação."]