{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":13,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSH-D / ERLA-DV37"]
[]
[]
[]
[]
["","","","","","EBSH16P30DF / ERLA16D2V37","EBSH16P50DF / ERLA16D2V37","EBSH16P30DF / ERLA16DAV37","EBSH16P50DF / ERLA16DAV37","EBSH16P50DG / ERLA16D2V37","EBSH16P30DG / ERLA16DAV37","EBSH16P30DG / ERLA16D2V37","EBSH16P50DG / ERLA16DAV37"]
["Indoor unit","","","","","EBSH16P30DF","EBSH16P50DF","EBSH16P30DF","EBSH16P50DF","EBSH16P50DG","EBSH16P30DG","EBSH16P30DG","EBSH16P50DG"]
["Capacidade de aquecimento","Nom.","","","kW","16.0 (1)","16.0 (1)","16.0 (1)","16.0 (1)","16.0","16.0","16.0","16.0"]
["Potência nominal","Aquecimento","","Nom.","kW","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)"]
["COP","","","","","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)"]
["Aquecimento de água quente sanitária","Geral","","Perfil de carga declarado","","L","XL","L","XL","XL","L","L","XL"]
["","Clima médio","","Classe de eficiência energética para aquecimento de água","","A+","A+","A+","A+","A+","A+","A+","A+"]
["Aquecimento de espaços","Clima médio, saída da água 55 °C","Geral","SCOP","","3.32","3.32","3.32","3.32","3.32","3.32","3.32","3.32"]
["","","","Classe de efic. sazonal de aquecimento de espaços","","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Clima médio, saída da água 35 °C","Geral","SCOP","","4.61","4.61","4.61","4.61","4.61","4.61","4.61","4.61"]
["","","","Classe de efic. sazonal de aquecimento de espaços","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Notas","","","","","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]