{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EDLA04-08E3V3"]
[]
[]
[]
[]
["","","","","","EDLA04E23V3","EDLA06E23V3","EDLA08E23V3"]
["Capacidade de aquecimento","Nom.","","","kW","4.30 (1), 4.60 (2)","6.00 (1), 5.90 (2)","7.50 (1), 7.80 (2)"]
["Capacidade do aquecedor","Escalão 1","","","kW","3","3","3"]
["Potência nominal","Aquecimento","","Nom.","kW","0.840 (1), 1.26 (2)","1.24 (1), 1.69 (2)","1.63 (1), 2.23 (2)"]
["COP","","","","","5.10 (1), 3.65 (2)","4.85 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["Dimensões","Unidade","","Altura","mm","770","770","770"]
["","","","Largura","mm","1250","1250","1250"]
["","","","Profundidade","mm","362","362","362"]
["Peso","Unidade","","","kg","91","91","91"]
["Limite de funcionamento","Aquecimento","Lado da água","Mín.","°C","15 (3)","15 (3)","15 (3)"]
["","","","Máx.","°C","65 (3)","65 (3)","65 (3)"]
["","Água doméstica quente","Ambiente","Mín.","°CBs","-27","-27","-27"]
["","","","Máx.","°CBs","35","35","35"]
["","","Lado da água","Mín.","°C","25","25","25"]
["","","","Máx.","°C","55 (3)","55 (3)","55 (3)"]
["Nível de potência sonora","Aquecimento","","Nom.","dBA","58.0 (1)","60.0 (1)","62.0 (1)"]
["Nível de pressão sonora","Aquecimento","","Nom.","dBA","44.0 (1)","47.0 (1)","49.0 (1)"]
["Fluido frigorigéneo","Tipo","","","","R-32","R-32","R-32"]
["","GWP","","","","675","675","675"]
["","Carga","","","kg","1.35","1.35","1.35"]
["","Carga","","","tCO2Eq","0.91","0.91","0.91"]
["Aquecimento de espaços","Clima médio, saída da água 55 °C","Geral","SCOP","","3.26","3.26","3.32"]
["","","","Classe de efic. sazonal de aquecimento de espaços","","A++","A++","A++"]
["","Clima médio, saída da água 35 °C","Geral","SCOP","","4.48","4.47","4.56"]
["","","","Classe de efic. sazonal de aquecimento de espaços","","A+++","A+++","A+++"]
["Componente do compressor","Alimentação eléctrica principal","","Fase","","3N","3N","3N"]
["","","","Tensão","V","220","220","220"]
["Alimentação elétrica","Nome","","","","V3","V3","V3"]
["","Fase","","","","1~","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50","50"]
["","Tensão","","","V","230 +/-10%","230 +/-10%","230 +/-10%"]
["Notas","","","","","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condição 2: arrefecimento Ta 35°C - LWE 7°C (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condição 2: arrefecimento Ta 35°C - LWE 7°C (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condição 2: arrefecimento Ta 35°C - LWE 7°C (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]
["","","","","","(3) - Para mais informações, consulte o desenho dos limites de funcionamento","(3) - Para mais informações, consulte o desenho dos limites de funcionamento","(3) - Para mais informações, consulte o desenho dos limites de funcionamento"]