{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSAX-D9W"]
[]
[]
[]
[]
["","","","","","EGSAX06DA9W","EGSAX10DA9W"]
["Capacidade de aquecimento","Mín.","","","kW","0.85","0.85"]
["","Nom.","","","kW","3.35","5.49"]
["","Máx.","","","kW","7.98","9.55"]
["Power input","Nom.","","","kW","0.74","1.17"]
["COP","","","","","4.51","4.70"]
["Envolvente","Cor","","","","Branco + Preto","Branco + Preto"]
["","Material","","","","Folha de metal revestida"]
["Dimensões","Unidade","","Width","mm","597","597"]
["","","","Depth","mm","666","666"]
["Peso","Unidade","","","kg","222","222"]
["Depósito","Volume de água","","","l","180"]
["","Isolamento","","Perda de calor","kWh/24h","1.2","1.2"]
["","Protecção contra corrosão","","","","Decapagem","Decapagem"]
["Fluido frigorigéneo","Type","","","","R-32","R-32"]
["","GWP","","","","675.0","675.0"]
["","Carga","","","kg","1.70","1.70"]
["Limite de funcionamento","Espaço de instalação","","Mín.","°C","5","5"]
["","","","Máx.","°C","35","35"]
["","Lado de salmoura","","Mín.","°C","-10","-10"]
["","","","Máx.","°C","30","30"]
["","Aquecimento","Lado da água","Mín.","°C","5","5"]
["","","","Máx.","°C","65","65"]
["","Água doméstica quente","Lado da água","Mín.","°C","25","25"]
["","","","Máx.","°C","60","60"]
["Aquecimento ambiente","Clima médio, saída da água 55 °C","Geral","SCOP","","3.77 (1)","4.05 (1)"]
["","","","Seasonal space heating eff. class","","A++","A+++"]
["","Clima médio, saída da água 35 °C","Geral","SCOP","","5.18 (1)","5.20 (1)"]
["","","","Classe de efic. sazonal de aquecimento de espaços","","A+++","A+++"]
["Power supply","Fase","","","","1~/3~","1~/3~"]
["","Frequência","","","Hz","50","50"]
["","Tensão","","","V","230/400","230/400"]
["Corrente","Fusíveis recomendados","","","A","16/32","16/32"]
["Notas","","","","","(1) - Em conformidade com as normas EN14825 e EN14511:2018","(1) - Em conformidade com as normas EN14825 e EN14511:2018"]
["","","","","","(2) - Consultar o esquema de intervalo de funcionamento: aumento de intervalo através de aquecimento de impulsionador de reserva ou aquecedor de reserva","(2) - Consultar o esquema de intervalo de funcionamento: aumento de intervalo através de aquecimento de impulsionador de reserva ou aquecedor de reserva"]