{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":7,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBH-E9W / ERGA-EVH7"]
[]
[]
[]
[]
["","","","","","EHBH08EA9W / ERGA08EAV3H7","EHBH08EF9W / ERGA08EAV3H7"]
["Capacidade de aquecimento","Nom.","","","kW","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Potência nominal","Aquecimento","","Nom.","kW","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["COP","","","","","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["Aquecimento de espaços","Clima médio, saída da água 55 °C","Geral","SCOP","","3.32","3.32"]
["","","","Classe de efic. sazonal de aquecimento de espaços","","A++","A++"]
["","Clima médio, saída da água 35 °C","Geral","SCOP","","4.56","4.56"]
["","","","Classe de efic. sazonal de aquecimento de espaços","","A+++","A+++"]
["Gama de eficiência energética","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notas","","","","","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condição 2: arrefecimento Ta 35°C - LWE 7°C (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condição 2: arrefecimento Ta 35°C - LWE 7°C (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]