{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBX-CB / ERHQ-BW17"]
[]
[]
[]
[]
["","","","","","EHBX16CB3V / ERHQ014BAW17","EHBX16CB9W / ERHQ014BAW17"]
["Capacidade de aquecimento","Nom.","","","kW","14.5 (1), 13.6 (2)","14.5 (1), 13.6 (2)"]
["Capacidade de arrefecimento","Nom.","","","kW","16.1 (1), 12.6 (2)","16.1 (1), 12.6 (2)"]
["Potência nominal","Aquecimento","","Nom.","kW","3.42 (1), 4.21 (2)","3.42 (1), 4.21 (2)"]
["","Arrefecimento","","Nom.","kW","5.43 (1), 5.08 (2)","5.43 (1), 5.08 (2)"]
["COP","","","","","4.24 (1), 3.22 (2)","4.24 (1), 3.22 (2)"]
["EER","","","","","2.96 (1), 2.47 (2)","2.96 (1), 2.47 (2)"]
["Aquecimento de espaços","Clima médio, saída da água 55 °C","Geral","SCOP","","2.86","2.86"]
["","","","Classe de efic. sazonal de aquecimento de espaços","","A+","A+"]
["","Clima médio, saída da água 35 °C","Geral","SCOP","","3.34","3.34"]
["","","","Classe de efic. sazonal de aquecimento de espaços","","A+","A+"]
["Gama de eficiência energética","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notas","","","","","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condição 2: arrefecimento Ta 35°C - LWE 7°C (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condição 2: arrefecimento Ta 35°C - LWE 7°C (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]
["","","","","","(3) - Tamb 35°C - LWE 7°C (DT=5°C)","(3) - Tamb 35°C - LWE 7°C (DT=5°C)"]
["","","","","","(4) - Tamb 35°C - LWE 18℃ (DT=5°C)","(4) - Tamb 35°C - LWE 18℃ (DT=5°C)"]
["","","","","","(5) - Bs/Bh 7°C/6°C-LWC 35°C(DT=5°C)","(5) - Bs/Bh 7°C/6°C-LWC 35°C(DT=5°C)"]
["","","","","","(6) - DB/WB 7°C/6°C - LWC 45℃ (Dt=5°C)","(6) - DB/WB 7°C/6°C - LWC 45℃ (Dt=5°C)"]