{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-D3"]
[]
[]
[]
[]
["","","","","","EHSX04P30DA3","EHSX04P50DA3","EHSX08P30DA3","EHSX08P50DA3"]
["Envolvente","Cor","","","","Branco (RAL9016)/Cinzento escuro (RAL7011)","Branco (RAL9016)/Cinzento escuro (RAL7011)","Branco (RAL9016)/Cinzento escuro (RAL7011)","Branco (RAL9016)/Cinzento escuro (RAL7011)"]
["","Material","","","","Polipropileno resistente ao impacto","Polipropileno resistente ao impacto","Polipropileno resistente ao impacto","Polipropileno resistente ao impacto"]
["Dimensões","Unidade","","Altura","mm","1891","1896","1891","1896"]
["","","","Largura","mm","595","790","595","790"]
["","","","Profundidade","mm","615","790","615","790"]
["Peso","Unidade","","","kg","73.0","93.0","73.0","93.0"]
["PED","Categoria","","","","art. 3,3","art. 3,3","art. 3,3","art. 3,3"]
["Fluido frigorigéneo","Tipo","","","","R-32","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0","675.0"]
["","Carga","","","kg","1.50","1.50","1.50","1.50"]
["Nível de potência sonora","Nom.","","","dBA","39","39","39","39"]
["Limite de funcionamento","Aquecimento","Lado da água","Mín.","°C","18","18","18","18"]
["","","","Máx.","°C","65","65","65","65"]
["","Arrefecimento","Ambiente","Mín.","° CBs","10","10","10","10"]
["","","Lado da água","Mín.","°C","5","5","5","5"]
["","","","Máx.","°C","22","22","22","22"]
["Alimentação elétrica","Fase","","","","1~","1~","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50","50","50"]
["","Tensão","","","V","230","230","230","230"]
["Aquecedor eléctrico","Alimentação eléctrica","","Nome","","3V / 9W","3V / 9W","3V / 9W","3V / 9W"]
["","","","Fase","","1~ / 3~","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Frequência","Hz","50","50","50","50"]
["Notas","","","","","(1) - Perda de calor de acordo com EN12897","(1) - Perda de calor de acordo com EN12897","(1) - Perda de calor de acordo com EN12897","(1) - Perda de calor de acordo com EN12897"]
["","","","","","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C"]
["","","","","","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60℃","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60℃","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60℃","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60℃"]
["","","","","","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65℃","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65℃","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65℃","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65℃"]
["","","","","","","(5) - Aquecimento do depósito apenas com bomba de calor, sem aquecedor elétrico","","(5) - Aquecimento do depósito apenas com bomba de calor, sem aquecedor elétrico"]