{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E6VG / ERGA-EV"]
[]
[]
[]
[]
["","","","","","EHVX04S18EA6VG / ERGA04EAV3","EHVX04S23EA6VG / ERGA04EAV3"]
["Capacidade de aquecimento","Nom.","","","kW","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)"]
["Capacidade de arrefecimento","Nom.","","","kW","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)"]
["Potência nominal","Aquecimento","","Nom.","kW","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)"]
["","Arrefecimento","","Nom.","kW","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)"]
["Potência absorvida","Água quente sanitária de 10°C a 50°C","","Nom.","kWh","2.48","3.01"]
["Tempo de aquecimento de 10°C a 50°C","hr","","","","1h28min","1h40min"]
["COP","","","","","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)"]
["EER","","","","","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)"]
["Aquecimento de água quente sanitária","Geral","","Perfil de carga declarado","","L","XL"]
["","Clima médio","","Classe de eficiência energética para aquecimento de água","","A+","A+"]
["Aquecimento de espaços","Clima médio, saída da água 55 °C","Geral","SCOP","","3.29","3.29"]
["","","","Classe de efic. sazonal de aquecimento de espaços","","A++","A++"]
["","Clima médio, saída da água 35 °C","Geral","SCOP","","4.54","4.54"]
["","","","Classe de efic. sazonal de aquecimento de espaços","","A+++","A+++"]
["Notas","","","","","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condição 1: arrefecimento Ta 35°C - LWE 18℃ (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condição 2: arrefecimento Ta 35°C - LWE 7°C (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condição 2: arrefecimento Ta 35°C - LWE 7°C (DT = 5°C); aquecimento Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]