{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AFV3"]
["Envolvente","Cor","","","","Branco"]
["","Material","","","","Folha de metal revestida"]
["Dimensões","Unidade","","Altura","mm","902"]
["","","","Largura","mm","450"]
["","","","Profundidade","mm","164"]
["Peso","Unidade","","","kg","31.2"]
["PED","Categoria","","","","Categoria I"]
["Permutador de calor lado da água","Caudal de água","Aquecimento","Máx.","l/min","23.5 (7)"]
["Nível de potência sonora","Nom.","","","dBA","42.0"]
["Limite de funcionamento","Aquecimento","Lado da água","Mín.","°C","25 (8)"]
["","","","Máx.","°C","55 (8)"]
["","Arrefecimento","Ambiente","Mín.","°CBs","10 (8)"]
["","","Lado da água","Mín.","°C","5 (8)"]
["","","","Máx.","°C","22 (8)"]
["Alimentação elétrica","Nome","","","","V3"]
["","Fase","","","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50"]
["","Tensão","","","V","230"]
["Ligações eléctricas","Para ligação à interface do utilizador","","Quantidade","","2"]
["","","","Observação","","0,75 mm² até 1,25 mm² (comprimento máx. 500m)"]
["Notas","","","","","(1) - Apenas para a unidade interior"]
["","","","","","(2) - Bs/Bh 7 °C/6 °C - LWC 35 °C (DT=5 °C), caldeira derivada"]
["","","","","","(3) - Bs/Bh 7 °C/6 °C - LWC 45℃ (DT=5 °C), caldeira derivada"]
["","","","","","(4) - Tamb 35°C - LWE 7°C (DT=5°C), derivação da caldeira"]
["","","","","","(5) - Tamb 35°C - LWE 18°C (DT=5°C), derivação da caldeira"]
["","","","","","(6) - Min. required"]
["","","","","","(7) - Caldeira derivada"]
["","","","","","(8) - Para os limites de funcionamento de *HYHB* e *HYKOMB33AA, consulte o esquema dos limites de funcionamento"]