{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":9,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKEQ"]
[]
[]
[]
[]
["","","","","EKEQDCBV3","EKEQMCBV3","EKEQMCBAV3","EKEQFCBAV3","EKEQFCBV3"]
["Outdoor unit","","","","ERQ","VRV","VRV","ERQ","ERQ"]
["Aplicação","","","","Par","Multi","Multi","Par","Par"]
["Dimensões","Unidade","Altura","mm","132","132","132","132","132"]
["","","Width","mm","400","400","400","400","400"]
["","","Depth","mm","200","200","200","200","200"]
["Peso","Unidade","","kg","3.6","3.6","3.6","3.9","3.9"]
["Limite de funcionamento","Arrefecimento","Mín.","° CBs","-10","-10","-10","-10","-10"]
["","","Máx.","° CBs","40","40","40","40","40"]
["Acessórios standard","Termistor (R1T)","","","1","1","1","0","0"]
["","Termistor (R2T/R3T)","","","2","2","2","2","2"]
["","Folha de isolamento","","","2","2","2","2","2"]
["","Folha de borracha","","","2","2","2","2","2"]
["","Junta de fio para fio","","","6","6","6","4","4"]
["","Manual de instalação e funcionamento","","","1","1","1","1","1"]
["","Porca do parafuso","","","8","9","9","7","7"]
["","Atilhos","","","6","6","6","6","6"]
["","Adaptador de definição de capacidade","","","7","8","8","7","7"]
["","Batente (a fechar)","","","0","0","0","2","2"]
["Power supply","Nome","","","V3","V3","V3","V3","V3"]
["","Fase","","","1~","1~","1~","1~","1~"]
["","Frequência","","Hz","50","50","50","50","50"]
["","Tensão","","V","230","230","230","230","230"]