{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHHP-A2V3 / ERWQ-AV3"]
[]
[]
[]
[]
["","","","","EKHHP300AA2V3 / ERWQ02AAV3","EKHHP500AA2V3 / ERWQ02AAV3","EKHHP300AC2V3 / ERWQ02AAV3","EKHHP500AC2V3 / ERWQ02AAV3","EKHHP300AB2V3 / ERWQ02AAV3 (Archived)","EKHHP500AB2V3 / ERWQ02AAV3 (Archived)"]
["Indoor unit","","","","EKHHP300AA2V3","EKHHP500AA2V3","EKHHP300AC2V3","EKHHP500AC2V3","EKHHP300AB2V3","EKHHP500AB2V3"]
["Aquecimento de água quente sanitária","Geral","Perfil de carga declarado","","L","XL","L","XL","L","XL"]
["","Clima médio","Classe de eficiência energética para aquecimento de água","","A+","A","A+","A+","A+","A+"]
["Gama de eficiência energética","","","","","","A+ ~ F","A+ ~ F","A+ ~ F","A+ ~ F"]