{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWP-PB"]
[]
[]
[]
[]
["","","","","","EKHWP300PB","EKHWP500PB"]
["Instalação_","","","","","Chão","Chão"]
["Envolvente","Cor","","","","Branco (RAL9016)/Cinzento escuro (RAL7011)","Branco (RAL9016)/Cinzento escuro (RAL7011)"]
["","Material","","","","Polipropileno resistente ao impacto","Polipropileno resistente ao impacto"]
["Dimensões","Unidade","Altura","Depósito","mm","1646","1658"]
["","","","Largura","mm","595","790"]
["","","","Profundidade","mm","615","790"]
["Peso","Unidade","","Vazio","kg","56","82"]
["","","","Total","kg","350","559"]
["Depósito","Volume de água","","","l","294","477"]
["","Material","","","","Polipropileno","Polipropileno"]
["","Temperatura máxima da água","","","°C","85","85"]
["","Classe de eficiência energética","","","","B","B"]
["Permutador de calor","Água doméstica quente","","Quantidade","","1","1"]
["","","","Material de tubo","","Aço inoxidável (DIN 1.4404)","Aço inoxidável (DIN 1.4404)"]
["","","","Volume da serpentina interna","l","27.8","29.0"]
["","","","Pressão de funcionamento","bar","10.0","10.0"]
["","Carregamento","","Quantidade","","1","1"]
["","","","Material de tubo","","Aço inoxidável (DIN 1.4404)","Aço inoxidável (DIN 1.4404)"]
["","","","Volume da serpentina interna","l","12.9","18.1"]
["","","","Pressão de funcionamento","bar","6.0","6.0"]
["","Aquecimento solar auxiliar","","Quantidade","","","1"]
["","","","Material de tubo","","","Aço inoxidável (DIN 1.4404)"]
["","","","Volume da serpentina interna","l","","3.9"]
["","","","Pressão de funcionamento","bar","","3.0"]
["Notas","","","","","(1) - Perda de calor de acordo com EN12897","(1) - Perda de calor de acordo com EN12897"]
["","","","","","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C"]
["","","","","","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60℃","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60℃"]
["","","","","","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65℃","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65℃"]
["","","","","","(5) - Para o volume de drenagem de 140 l -> 5820 Wh (banho)/8 kW, bomba de calor","(5) - Para o volume de drenagem de 140 l -> 5820 Wh (banho)/16 kW, bomba de calor"]
["","","","","","(6) - Para o volume de drenagem de 90 l -> 3660 Wh (banho)/8 kW, bomba de calor","(6) - Para o volume de drenagem de 90 l -> 3660 Wh (banho)/16 kW, bomba de calor"]