{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":5,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKRTW"]
[]
[]
[]
[]
["","","","","EKRTWA"]
["Função de regulação","","","","Banda proporcional"]
["Dimensões","Unidade","Width","mm","125"]
["","","Depth","mm","34"]
["","","Altura","mm","87"]
["Limites de definição da temperatura","Aquecimento","Máx.","°C","37"]
["","","Mín.","°C","4"]
["","Arrefecimento","Máx.","°C","37"]
["","","Mín.","°C","4"]
["Relógio","","","","Sim"]
["Peso","Unidade","","g","215"]
["Temperatura ambiente","Armazenamento","Mín.","°C","-20"]
["","","Máx.","°F","140"]
["","","Mín.","°F","-4"]
["","","Máx.","°C","60"]
["","Funcionamento","Mín.","°C","0"]
["","","Máx.","°F","122"]
["","","Mín.","°F","32"]
["","","Máx.","°C","50"]
["Corrente de comutação máxima (a 230 VAC)","A","","","5.0 (1)"]
["Ligação","Tipo","","","Com fios"]
["Power supply","Tensão","","V","Alimentado a pilhas 3* AA-LR6 (alcalinas)"]
["Notas","","","","(1) - 230VAC"]