{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKSRPS4A"]
[]
[]
[]
[]
["","","","","EKSRPS4AB","EKSRPS4A."]
["Temperatura em inactividade","Máx.","","°C","85","85"]
["Dimensões","Unidade","Width","mm","142","142"]
["","","Depth","mm","230","230"]
["","","Altura","mm","815","815"]
["Peso","Unidade","","kg","6.4","6"]
["Limite de funcionamento","Temperatura ambiente","Máx.","°C","40","40"]
["","","Mín.","°C","5","5"]
["Pressão de funcionamento","Máx.","","bar","0"]
["Instalação_","","","","Na lateral do depósito","Na lateral do depósito"]
["Power supply intake","","","","Unidade interior","Unidade interior"]
["Controlo","Tipo","","","Controlador de diferença de temperatura digital com apresentação de texto plano","Controlador de diferença de temperatura digital com apresentação de texto plano"]
["","Consumo de energia","","W","2","2"]
["Power supply","Fase","","","1~","1~"]
["","Frequência","","Hz","50","50"]
["","Tensão","","V","230","230"]