{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSK12-14AW1"]
[]
[]
[]
[]
["","","","","","EPSK12ARW1","EPSK14ARW1"]
["Dimensões","Unidade","","Altura","mm","1,123","1,123"]
["","","","Largura","mm","1,330","1,330"]
["","","","Profundidade","mm","604","604"]
["Peso","Unidade","","","kg","191","191"]
["Ventilador","Caudal de ar","Aquecimento","Alto","m³/min","96.3","96.3"]
["","","Arrefecimento","Alto","m³/min","96.3","96.3"]
["Limites&nbsp;de&nbsp;funcionamento","Limites&nbsp;de&nbsp;funcionamento-=-Arrefecimento","","Limites&nbsp;de&nbsp;funcionamento-=-Arrefecimento-=-Mín.-=-°CBs","° CBs","10","10"]
["","","","Limites&nbsp;de&nbsp;funcionamento-=-Arrefecimento-=-Máx.-=-°CBs","° CBs","43","43"]
["Limite de funcionamento","Água doméstica quente","","Mín.","° CBs","-28","-28"]
["Limites&nbsp;de&nbsp;funcionamento","Limites&nbsp;de&nbsp;funcionamento-=-Água quente sanitária","","Limites&nbsp;de&nbsp;funcionamento-=-Água quente sanitária-=-Máx.-=-°CBs","° CBs","40","40"]
["Nível de potência sonora","Aquecimento","","Nom.","dBA","52 (1)","52 (1)"]
["","Arrefecimento","","Nom.","dBA","62 (2)","63 (2)"]
["Nível de pressão sonora","Aquecimento","","Nom.","dBA","38 (1)","38 (1)"]
["","Arrefecimento","","Nom.","dBA","47 (2)","48 (2)"]
["Fluido frigorigéneo","Tipo","","","","R-290","R-290"]
["","GWP","","","","3","3"]
["","Carga","","","tCO2Eq","0.0038","0.0038"]
["","Carga","","","kg","1.25","1.25"]
["Ligações de tubagens","Diferença de nível","IU - OU","Máx.","m","10","10"]
["Alimentação elétrica","Nome","","","","W1","W1"]
["","Fase","","","","3~","3~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50"]
["","Tensão","","","V","400","400"]
["Palavra-passe","Fusíveis recomendados","","","A","16","16"]
["Notas","","","","","(1) - Medido a LWC 47-55°C; Ta DB/WB 7 °C/6 °C.","(1) - Medido a LWC 47-55°C; Ta DB/WB 7 °C/6 °C."]
["","","","","","(2) - Medido a LWC 12-7 °C; Ta 35 °C.","(2) - Medido a LWC 12-7 °C; Ta 35 °C."]
["","","","","","(3) - Tubagem no terreno 1 1/4\"","(3) - Tubagem no terreno 1 1/4\""]
["","","","","","(4) - Tubagem no terreno 1 1/2\"","(4) - Tubagem no terreno 1 1/2\""]