{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSXB14A"]
[]
[]
[]
[]
["","","","","","EPSXB14P30AF","EPSXB14P50AF"]
["Envolvente","Cor","","","","Branco Traffic (RAL9016), Preto Graphite (RAL9011), Preto Jet (RAL9005)","Branco Traffic (RAL9016), Preto Graphite (RAL9011), Preto Jet (RAL9005)"]
["","Material","","","","Polipropileno resistente ao impacto","Polipropileno resistente ao impacto"]
["Dimensões","Unidade","","Altura","mm","1914","1906"]
["","","","Largura","mm","590","785"]
["","","","Profundidade","mm","671","837"]
["Peso","Unidade","","","kg","87.0","109"]
["PED","Categoria","","","","Art4.3","Art4.3"]
["Nível de potência sonora","Nom.","","","dBA","49.0","49.0"]
["Nível de pressão sonora","Nível de pressão sonora-=-Nom.-=-dBA","","","dBA","35.0","35.0"]
["Limite de funcionamento","Aquecimento","Lado da água","Mín.","°C","0 (3)","0 (3)"]
["","","","Máx.","°C","0 (3)","0 (3)"]
["","Arrefecimento","Ambiente","Mín.","° CBs","0 (3)","0 (3)"]
["","","Lado da água","Mín.","°C","0 (3)","0 (3)"]
["","","","Máx.","°C","0 (3)","0 (3)"]
["Alimentação elétrica","Fase","","","","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50"]
["","Tensão","","","V","230","230"]
["Aquecedor eléctrico","Alimentação eléctrica","","Nome","","6V / 9W","6V / 9W"]
["","","","Fase","","1~ / 3~","1~ / 3~"]
["","","","Frequência","Hz","50","50"]
["","","","Tensão","V","230/400","230/400"]
["","Fusíveis recomendados","","","A","0 (4)","0 (4)"]
["Notas","","","","","(1) - Perda de calor de acordo com EN12897","(1) - Perda de calor de acordo com EN12897"]
["","","","","","(2) - Volume mínimo necessário, excluindo o volume na unidade","(2) - Volume mínimo necessário, excluindo o volume na unidade"]
["","","","","","(3) - Consultar a imagem dos limites de funcionamento","(3) - Consultar a imagem dos limites de funcionamento"]
["","","","","","(4) - Consulte o diagrama de cablagem e o manual de instalação para o fusível recomendado correto, consoante a alimentação elétrica e a ligação de rede","(4) - Consulte o diagrama de cablagem e o manual de instalação para o fusível recomendado correto, consoante a alimentação elétrica e a ligação de rede"]