{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERSQ-AY1"]
[]
[]
[]
[]
["","","","","","ERSQ011AAY1","ERSQ014AAY1","ERSQ016AAY1"]
["Nível de pressão sonora","Aquecimento","","Nom.","dBA","52","53","55"]
["Acessórios standard","Manual de instalação","","","","1","1","1"]
["Fluido frigorigéneo","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Carga","","","kg","4.5","4.5","4.5"]
["","Type","","","","R-410A","R-410A","R-410A"]
["Limite de funcionamento","Aquecimento","","Máx.","° CBh","20","20","20"]
["","","","Mín.","° CBh","-20","-20","-20"]
["","Água doméstica quente","","Mín.","° CBs","-20","-20","-20"]
["","","","Máx.","° CBs","35","35","35"]
["Piping connections","Isolamento de calor","","","","Tubos de líquidos e gás","Tubos de líquidos e gás","Tubos de líquidos e gás"]
["","Liquid","","OD","mm","9.52","9.52","9.52"]
["","Gás","","OD","mm","15.9","15.9","15.9"]
["","Drain","","OD","mm","26x3","26x3","26x3"]
["","Diferença de nível","IU - OU","Máx.","m","30","30","30"]
["Nível de potência sonora","Aquecimento","","Nom.","dBA","68","69","71"]
["Dimensões","Unidade","","Width","mm","900","900","900"]
["","","","Depth","mm","320","320","320"]
["","","","Altura","mm","1,345","1,345","1,345"]
["Peso","Unidade","","","kg","120","120","120"]
["Power supply","Fase","","","","3~","3~","3~"]
["","Nome","","","","Y1","Y1","Y1"]
["","Frequência","","","Hz","50","50","50"]
["","Tensão","","","V","380-415","380-415","380-415"]
["Corrente","Fusíveis recomendados","","","A","16","16","16"]
["Notas","","","","","(1) - Consulte o esquema separado para conhecer os limites de funcionamento","(1) - Consulte o esquema separado para conhecer os limites de funcionamento","(1) - Consulte o esquema separado para conhecer os limites de funcionamento"]
["","","","","","(2) - Ssc: potência de curto-circuito","(2) - Ssc: potência de curto-circuito","(2) - Ssc: potência de curto-circuito"]
["","","","","","(3) - Contém gases fluorados com efeito de estufa","(3) - Contém gases fluorados com efeito de estufa","(3) - Contém gases fluorados com efeito de estufa"]