{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERWQ-AV3"]
[]
[]
[]
[]
["","","","","","ERWQ02AAV3"]
["Dimensões","Unidade","","Altura","mm","550"]
["","","","Largura","mm","765"]
["","","","Profundidade","mm","285"]
["Peso","Unidade","","","kg","35"]
["Limites de funcionamento","Água doméstica quente","","Máx.","°CBs","35"]
["","","","Mín.","°CBs","-15"]
["Piping connections","Líquido","","DE","mm","6.35"]
["","Gás","","DE","mm","9.5"]
["","Diferença de nível","IU - OU","Máx.","m","15"]
["Nível de pressão sonora","Aquecimento","","Nom.","dBA","47"]
["","Arrefecimento","","Nom.","dBA","47"]
["Fluido frigorigéneo","Tipo","","","","R-410A"]
["","GWP","","","","2,087.5"]
["","Carga","","","kg","1.05"]
["Power supply","Nome","","","","V3"]
["","Phase","","","","1~"]
["","Frequência","","","Hz","50"]
["","Tensão","","","V","230"]
["Notas","","","","","(1) - Contém gases fluorados com efeito de estufa"]