{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSX-D"]
[]
[]
[]
[]
["","","","","","ETSX16P30DA","ETSX16P50DA"]
["Nível de pressão sonora","Nom.","","","dBA","32.8","32.8"]
["Limites de funcionamento","Arrefecimento","Ambiente","Mín.","°CBs","10","10"]
["","","Lado da água","Máx.","°C","22","22"]
["","","","Mín.","°C","5","5"]
["","Aquecimento","Lado da água","Máx.","°C","70","70"]
["","","","Min.","°C","15","15"]
["Nível de potência sonora","Nom.","","","dBA","45.6","45.6"]
["Dimensões","Unidade","","Largura","mm","590","785"]
["","","","Profundidade","mm","615","785"]
["","","","Altura","mm","1,891","1,896"]
["Envolvente","Material","","","","Polipropileno resistente ao impacto","Polipropileno resistente ao impacto"]
["","Colour","","","","Branco (RAL9016)/Cinzento escuro (RAL7011)","Branco (RAL9016)/Cinzento escuro (RAL7011)"]
["PED","Categoria","","","","Art4.3","Art4.3"]
["Peso","Unidade","","","kg","73","90"]
["Power supply","Phase","","","","1~","1~"]
["","Frequência","","","Hz","50","50"]
["","Tensão","","","V","230","230"]
["Aquecedor eléctrico","Alimentação eléctrica","","Frequência","Hz","50","50"]
["","","","Nome","","3V / 9W","3V / 9W"]
["","","","Fase","","1~ / 3~","1~ / 3~"]
["Notas","","","","","(1) - Perda de calor de acordo com EN12897","(1) - Perda de calor de acordo com EN12897"]
["","","","","","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C"]
["","","","","","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60℃","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60℃"]
["","","","","","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65℃","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65℃"]