{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWYT-CZO"]
[]
[]
[]
[]
["","","","","","EWYT021CZO-A1","EWYT032CZO-A1","EWYT040CZO-A1","EWYT064CZO-A2"]
["Dimensões","Unidade","","Altura","mm","1,878","1,878","1,878","1,878"]
["","","","Largura","mm","1,152","1,752","1,752","2,906"]
["","","","Profundidade","mm","802","802","802","814"]
["Peso","Unidade","","","kg","265","357","357","620"]
["Nível de potência sonora","Arrefecimento","","Nom.","dBA","76.0","79.0","80.0","83.0"]
["Nível de pressão sonora","Arrefecimento","","Nom.","dBA","59.6","62.2","63.2","65.4"]
["Fluido frigorigéneo","GWP","","","","675.0","675.0","675.0","675.0"]
["","Carga","","","tCO2Eq","4,928.0","6,422.0","6,635.0","11,255.0"]
["","Carga","","","kg","7.3","9.5","9.8","16.6"]
["Ligações de tubagem","Líquido","","DE","mm","28.6","28.6","28.6","28.6"]
["","Gás","","DE","mm","9.52","12.7","12.7","12.7, 9.52"]
["Ligações de tubagens","Diferença de nível","IU - OU","Máx.","m","10.0","10.0","10.0","10.0"]
["Alimentação eléctrica","Frequência","","","Hz","50","50","50","50"]