{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Envolvente","Cor","","","","Branco","Branco"]
["","Material","","","","Resina","Resina"]
["Dimensões","Unidade","","Altura","mm","290","340"]
["","","","Largura","mm","1050","1200"]
["","","","Profundidade","mm","269","262"]
["Peso","Unidade","","","kg","14","18"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","16.2","23"]
["","","","Médio","m³/min","13.4","21.1"]
["","","","B","m³/min","12.1","18.7"]
["","","Aquecimento","Alto","m³/min","16.9","23"]
["","","","Médio","m³/min","14.2","20.9"]
["","","","B","m³/min","12.7","18.7"]
["Nível de potência sonora","Arrefecimento","","","dBA","61","65"]
["","Aquecimento","","","dBA","61","65"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","45","49"]
["","","","Médio","dBA","42","45"]
["","","","B","dBA","40","41"]
["","Aquecimento","","Alto","dBA","45","49"]
["","","","Médio","dBA","42","45"]
["","","","B","dBA","40","41"]
["Ligações de tubagem","Líquido","","DE","mm","9.52","9.52"]
["","Gás","","DE","mm","15.9","15.9"]
["","Esgoto","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Alimentação elétrica","Fase","","","","1~","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50","50"]
["","Tensão","","","V","220-240","220-240"]
["Acessórios standard","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Notas","","","","","(1) - As capacidades de arrefecimento nominais são baseadas em: temp. interior: 27 °CBs, 19 °CBh, temperatura exterior: 35 °CBs, tubagem de fluido frigorigéneo equivalente: 5 m, desnível: 0 m."]
["","","","","","(2) - As capacidades nominais de aquecimento são baseadas em: temperatura interior: 20°CBs, temperatura exterior: 7°CBs, 6°CBh, tubagem de refrigerante equivalente: 5m, diferença de nível: 0m."]
["Acessórios standard","Screw cover","","","","","3"]