{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RXM-A"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / RXM50A5V1B","FBA60A2VEB9 / RXM60A5V1B"]
["Capacidade de arrefecimento","Nom.","","kW","5.0","5.7"]
["Capacidade de aquecimento","Nom.","","kW","5.5","7"]
["Eficiência nominal","EER","","","3.55","3.48"]
["","COP","","","3.83","3.71"]
["","Consumo anual de energia","","kWh","704","819"]
["","Diretiva de etiqueta da energia","Arrefecimento","","A","A"]
["","","Aquecimento","","A","A"]
["Arrefecimento ambiente","Classe de eficiência energética","","","A++","A+"]
["","Capacidade","Pdesign","kW","5.0","5.7"]
["","SEER","","","6.27","5.91"]
["","Consumo anual de energia","","kWh/a","279","336"]
["Aquecimento ambiente (clima médio)","Classe de eficiência energética","","","A+","A+"]
["","Capacidade","Pdesign","kW","4.4","4.6"]
["","SCOP/A","","","4.06","4.01"]
["","Capacidade de aquecimento Pdh a -10°","","kW","3.73","3.99"]
["","Consumo anual de energia","","kWh/a","1,517","1607"]
["Notas","","","","","(1) - As capacidades de arrefecimento nominais são baseadas em: temp. interior: 27 °CBs, 19 °CBh, temperatura exterior: 35 °CBs, tubagem de fluido frigorigéneo equivalente: 5 m, desnível: 0 m."]
["","","","","","(2) - As capacidades nominais de aquecimento são baseadas em: temperatura interior: 20°CBs, temperatura exterior: 7°CBs, 6°CBh, tubagem de refrigerante equivalente: 5m, diferença de nível: 0m."]
["","","","","","(3) - Consulte o esquema separado para conhecer os limites de funcionamento"]
["","","","","","(4) - Consulte o esquema separado para conhecer os dados eléctricos"]