{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":10,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RZAG-A"]
[]
[]
[]
[]
["","","","","FBA35A2VEB9 / RZAG35A2V1B","FBA50A2VEB9 / RZAG50A2V1B","FBA60A2VEB9 / RZAG60A2V1B","FBA60A2VEB9 / RZAG50A2V1B","FBA71A2VEB9 / RZAG60A2V1B"]
["Capacidade de arrefecimento","Mín.","","kW","1.6","1.7","1.7","1.7","1.7"]
["","Máx.","","kW","5.0","6.0","7.0","6.0","7.0"]
["","Nom.","","kW","3.5","5.0","6.0","5.0","6.00"]
["Arrefecimento ambiente","SEER","","","6.12","6.30","6.15","6.63","6.25"]
["","Consumo anual de energia","","kWh/a","200","278","341","264","336"]
["","Capacidade","Pdesign","kW","3.50","5.00","6.00","5.00","6.00"]
["","Classe de eficiência energética","","","A++","A++","A++","A++","A++"]
["Aquecimento ambiente (clima médio)","Capacidade","Pdesign","kW","4.20","4.30","4.50","4.30","4.50"]
["","SCOP/A","","","4.10","4.10","4.10","4.28","4.18"]
["","Classe de eficiência energética","","","A+","A+","A+","A+","A+"]
["","Consumo anual de energia","","kWh/a","1,434","1,469","1,537","1,406","1,508"]
["Eficiência nominal","Consumo anual de energia","","kWh","389","625","741","608","696"]
["","EER","","","4.50","4.00","4.05","4.11","4.31"]
["","COP","","","4.40","3.80","3.80","3.97","3.87"]
["","Diretiva de etiqueta da energia","Arrefecimento","","A","A","A","A","A"]
["","","Aquecimento","","A","A","C","A","A"]
["Capacidade de aquecimento","Nom.","","kW","4.00","6.00","7.00","6.00","7.00"]
["","Mín.","","kW","1.40","1.70","1.70","1.70","1.70"]
["","Máx.","","kW","5.00","6.00","7.50","6.00","7.50"]
["Gama de eficiência energética","","","","","","","","","A+++ ~ D"]