{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RQ-BV3"]
[]
[]
[]
[]
["","","","","FCAG71AVEB / RQ71B8V3B","FCAG100AVEB / RQ100B8V3B"]
["Capacidade de arrefecimento","Nom.","","kW","7.10 (1)","10.0 (1)"]
["Eficiência nominal","EER","","","2.64","2.61"]
["","Consumo anual de energia","","kWh","1,345","1,915"]
["","COP","","","2.84","2.99"]
["","Diretiva de etiqueta da energia","Arrefecimento","","D","D"]
["","","Aquecimento","","D","D"]
["Capacidade de aquecimento","Nom.","","kW","8.00 (2)","11.2 (2)"]
["Notas","","","","(1) - Arrefecimento: temp. interior: 27°CBs, 19,0°CBh; temp. exterior 35°CBs; comprimento de tubagem equivalente: 5m; desnível: 0m","(1) - Arrefecimento: temp. interior: 27°CBs, 19,0°CBh; temp. exterior 35°CBs; comprimento de tubagem equivalente: 5m; desnível: 0m"]
["","","","","(2) - Aquecimento: temp. interior: 20°CBs; temp. exterior 7°CBs, 6°CBh; tubagem de refrigerante equivalente: 5m; desnível: 0m","(2) - Aquecimento: temp. interior: 20°CBs; temp. exterior 7°CBs, 6°CBh; tubagem de refrigerante equivalente: 5m; desnível: 0m"]