{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":13,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100HVEB / RZQG100L8Y1B","FCAHG125HVEB / RZQG125L8Y1B","FCAHG140HVEB / RZQG100L8Y1B","FCAHG140HVEB / RZQG125L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG100L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG125L8Y1B","FCAHG100HVEB / RZQG71L8Y1B","FCAHG71HVEB / RZQG71L8Y1B","FCAHG140HVEB / RZQG140L7Y1B"]
["Gama de eficiência energética","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Capacidade de arrefecimento","Nom.","","kW","","","","","","","6.80","6.80","13.40"]
["Arrefecimento ambiente","SEER","","","","","","","","","6.91","6.91","6.75"]
["","Consumo anual de energia","","kWh/a","","","","","","","345","345","1,191"]
["","Capacidade","Pdesign","kW","","","","","","","6.80","6.80","13.40"]
["","Classe de eficiência energética","","","","","","","","","A++","A++"]
["Aquecimento ambiente (clima médio)","Capacidade","Pdesign","kW","","","","","","","7.60","7.60","11.78"]
["","SCOP/A","","","","","","","","","4.54","4.54","4.38"]
["","Classe de eficiência energética","","","","","","","","","A+","A+"]
["","Consumo anual de energia","","kWh/a","","","","","","","2,344","2,344","3,766"]
["Eficiência nominal","EER","","","","","","","","","4.09","4.09","3.18"]
["Notas","","","","","","","","","","(1) - Consulte o esquema separado para conhecer os limites de funcionamento","(1) - As capacidades de arrefecimento nominais são baseadas em: temperatura interior: 27 °CBs, 19 °CBh, temperatura exterior: 35 °CBs, tubagem de fluido frigorigéneo equivalente: 5 m, desnível: 0 m.","(1) - As capacidades de arrefecimento nominais são baseadas em: temperatura interior: 27 °CBs, 19 °CBh, temperatura exterior: 35 °CBs, tubagem de fluido frigorigéneo equivalente: 5 m, desnível: 0 m."]
["","","","","","","","","","","(2) - Consulte o esquema separado para conhecer os dados eléctricos","(2) - As capacidades nominais de aquecimento são baseadas em: temperatura interior: 20°CBs, temperatura exterior: 7°CBs, 6°CBh, tubagem de refrigerante equivalente: 5m, diferença de nível: 0m.","(2) - As capacidades nominais de aquecimento são baseadas em: temperatura interior: 20°CBs, temperatura exterior: 7°CBs, 6°CBh, tubagem de refrigerante equivalente: 5m, diferença de nível: 0m."]
["Eficiência nominal","Annual energy consumption","","kWh","","","","","","","","831"]
["","COP","","","","","","","","","","4.80","4.12"]
["","Diretiva de etiqueta da energia","Arrefecimento","","","","","","","","","A"]
["","","Aquecimento","","","","","","","","","A"]
["Capacidade de aquecimento","Nom.","","kW","","","","","","","","7.50","15.50"]
["Notas","","","","","","","","","","","(3) - Consulte o esquema separado para conhecer os limites de funcionamento","(3) - Consulte o esquema separado para conhecer os limites de funcionamento"]
["","","","","","","","","","","","(4) - Consulte o esquema separado para conhecer os dados eléctricos","(4) - Consulte o esquema separado para conhecer os dados eléctricos"]
["Arrefecimento ambiente","ηs,c","","%","","","","","","","","","266.88"]
["Aquecimento ambiente (clima médio)","ηs,h","","%","","","","","","","","","172.10"]