{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FCQG71FVEB / RZQG71L9V1B","FCQG125FVEB / RZQG125L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG125L9V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG125L9V1B","FCQG71FVEB / FCQG71FVEB / RZQG125L9V1B","FCQG140FVEB / RZQG140L9V1B"]
["Capacidade de arrefecimento","Nom.","","kW","6.8","12.0","","","","13.4"]
["Arrefecimento ambiente","SEER","","","6.72","6.00","5.10","5.10","5.10"]
["","Consumo anual de energia","","kWh/a","355","700","824","824","824"]
["","Capacidade","Pdesign","kW","6.80","12.00","12.00","12.00","12.00"]
["","Classe de eficiência energética","","","A++","A+","B","B","B"]
["Aquecimento ambiente (clima médio)","Capacidade","Pdesign","kW","6.33","12.66","12.71","12.71","12.71"]
["","SCOP/A","","","4.20","4.10","3.80","3.80","3.80"]
["","Classe de eficiência energética","","","A+","A+","A","A","A"]
["","Consumo anual de energia","","kWh/a","2,110","4,323","4,683","4,683","4,683"]
["Eficiência nominal","Annual energy consumption","","kWh","1,005","1,610"]
["","EER","","","3.39","3.73","","","","3.21"]
["","COP","","","3.97","3.63","","","","3.61"]
["","Diretiva de etiqueta da energia","Arrefecimento","","A","A"]
["","","Aquecimento","","A","A"]
["Capacidade de aquecimento","Nom.","","kW","7.5","13.5","","","","15.5"]
["Notas","","","","(1) - Consumo anual de energia de acordo com a directiva de etiquetagem de energia 2002/31/EC","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE","","","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE"]
["","","","","(2) - SEER e SCOP de acordo com a EN 14825","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal","","","","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal"]