{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Nível de pressão sonora","Aquecimento","","Alto","dBA","35.0","35.0"]
["","","","B","dBA","29.0","29.0"]
["","Arrefecimento","","B","dBA","28.0","28.0"]
["","","","Alto","dBA","35.0","35.0"]
["Acessórios standard","Manual de instalação e funcionamento","","","","1","1"]
["","Filtro de ar de aspiração","","","","1","1"]
["Sistemas de controlo","Controlo remoto por cabo","","","","BRC1D52, BRC1E52A/B"]
["Ligações de tubagens","Liquid","","OD","mm","6.35"]
["","Gás","","OD","mm","9.52"]
["","Drain","","","","27.2"]
["Sound power level","Arrefecimento","","","dBA","55","55"]
["","Aquecimento","","","dBA","55","55"]
["Dimensões","Unidade","","Largura","mm","652","652"]
["","","","Profundidade","mm","502","502"]
["","","","Altura","mm","230","230"]
["Envolvente","Material","","","","Aço de baixo carbono revestido a zinco","Aço de baixo carbono revestido a zinco"]
["Peso","Unidade","","","kg","17.0","17.0"]
["Ventilador","Caudal de ar","Aquecimento","Alto","m³/min","","6.95"]
["","","","B","m³/min","","5.20"]
["","","Arrefecimento","B","m³/min","","5.20"]
["","","","Alto","m³/min","","6.50"]
["Power supply","Fase","","","","1~","1~"]
["","Frequência","","","Hz","50","50"]
["","Nome","","","","V1","V1"]
["","Tensão","","","V","230","230 +/-10%"]
["Notas","","","","","(1) - Os valores sonoros são medidos numa sala semi-anecóica.","(1) - Os valores sonoros são medidos numa sala semi-anecóica."]
["","","","","","(2) - O nível de pressão sonora é um valor relativo que depende da distância e acústica do ambiente. Para mais informações, consulte os esquemas do nível sonoro.","(2) - O nível de pressão sonora é um valor relativo que depende da distância e acústica do ambiente. Para mais informações, consulte os esquemas do nível sonoro."]
["","","","","","(3) - O nível de potência sonora é um valor absoluto que indica a potência que gera um determinado som.","(3) - O nível de potência sonora é um valor absoluto que indica a potência que gera um determinado som."]
["Ligações de tubagens","Liquid","","OD","mm","","6.35"]
["","Gás","","OD","mm","","9.52"]
["","Drain","","","","","27.2"]