{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FDQ125C5VEB / RZQSG125L9V1B (Archived)","FDQ125C7VEB / RZQSG125L9V1B (Archived)"]
["Capacidade de arrefecimento","Nom.","","kW","12.0","12.0"]
["Capacidade de aquecimento","Nom.","","kW","13.5","13.5"]
["Eficiência nominal","EER","","","3.21","3.21"]
["","COP","","","3.51","3.51"]
["","Annual energy consumption","","kWh","1,870","1,870"]
["","Diretiva de etiqueta da energia","Arrefecimento","","A","A"]
["","","Aquecimento","","B","B"]
["Arrefecimento ambiente","Classe de eficiência energética","","","A","A"]
["","Capacidade","Pdesign","kW","12.00","12.00"]
["","SEER","","","5.20","5.20"]
["","Consumo anual de energia","","kWh/a","808","808"]
["Aquecimento ambiente (clima médio)","Classe de eficiência energética","","","A","A"]
["","Capacidade","Pdesign","kW","7.60","7.60"]
["","SCOP/A","","","3.90","3.90"]
["","Consumo anual de energia","","kWh/a","2,729","2,729"]
["Notas","","","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE"]
["","","","","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal"]