{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":7,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F / 3MXM-M"]
[]
[]
[]
[]
["","","","","FDXM25F2V1B / FDXM25F2V1B / 3MXM40M2V1B","FDXM25F2V1B / FDXM35F2V1B / 3MXM40M2V1B","FDXM35F2V1B / FDXM35F2V1B / 3MXM40M2V1B"]
["Capacidade de arrefecimento","Nom.","","kW","4.00","4.00","4.00"]
["Eficiência nominal","Consumo anual de energia","","kWh","498","505","500"]
["","EER","","","4.02","3.96","4.00"]
["","COP","","","3.61","3.65","3.95"]
["","Diretiva de etiqueta da energia","Arrefecimento","","A","A","A"]
["","","Aquecimento","","A","A","A"]
["Capacidade de aquecimento","Nom.","","kW","4.60","4.60","4.60"]
["Notas","","","","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE","(1) - EER/COP de acordo com Eurovent 2012, para utilização exclusivamente fora da UE"]
["","","","","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal","(2) - Eficiência nominal: arrefecimento a 35°/27° de carga nominal, aquecimento a 7°/20° de carga nominal"]